{"text_format":"2","workbook":"xls","n_sheets":14,"sheets":["Figure 6","Figure 7","Figure 8","Figure 10","Figure 11","Figure 15","Figure 16","Figure 17","Figure 18","Figure 19","Figure 20","Figure 21","Figure 29","Figure 30"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Figure 6","index":0,"n_rows":156,"n_cols":11,"rows_kept":156,"cut":false,"hidden":false,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["FIG.6. Computed response in two anchor section, Texas A&M excavation, prior to SelfSim learning"]
[]
[{"$nulls":8},"Settlements (mm)"]
[null,"Settlements (mm)",{"$nulls":6},"Measured"]
[null,null,"Computed ",null,null,"Stage2",null,"Stage 4",null,"Stage 7"]
["Distance from the wall (m)","Stage 2","Stage 4","Stage 7",null,"Distance from the wall(m)","Settlemetns(mm)","Distance from the wall(m)","Settlemetns(mm)","Distance from the wall(m)","Settlemetns(mm)"]
[0,1.95,2.46,1.7,null,4.6604,-0.762,0.95402,2.794,0,21.844]
[0.0086868,1.92,2.42,1.66,null,7.9431,-1.651,4.6604,-1.016,1.8623,21.59]
[0.019568,1.89,2.37,1.62,null,9.7841,-1.9304,7.9431,-2.794,4.6604,3.9878]
[0.033162,1.85,2.33,1.57,null,14.966,0.254,9.7841,-2.54,7.9431,-3.81]
[0.049987,1.82,2.27,1.51,null,null,null,14.966,0,9.7841,-1.2446]
[0.071323,1.78,2.21,1.46,{"$nulls":5},14.966,-0.254]
[0.097841,1.73,2.15,1.39]
[0.13106,1.69,2.09,1.33]
[0.17252,1.64,2.02,1.26]
[0.22433,1.6,1.95,1.19]
[0.28926,1.55,1.87,1.11]
[0.36881,1.49,1.79,1.03]
[0.46939,1.43,1.7,0.948]
[0.59741,1.37,1.61,0.856]
[0.7559,1.29,1.5,0.761]
[0.95402,1.21,1.39,0.66]
[1.2009,1.11,1.28,0.557]
[1.4996,1.01,1.16,0.451]
[1.8959,0.886,1.02,0.343]
[2.3774,0.757,0.882,0.237]
[2.9809,0.615,0.721,0.128]
[3.7338,0.468,0.55,0.0273]
[4.6769,0.315,0.356,-0.081]
[5.8564,0.169,0.164,-0.178]
[7.3286,0.0415,-0.0178,-0.283]
[9.1696,-0.0577,-0.163,-0.362]
[11.471,-0.119,-0.254,-0.413]
[14.348,-0.142,-0.281,-0.407]
[17.945,-0.133,-0.258,-0.358]
[22.441,-0.101,-0.194,-0.269]
[28.061,-0.067,-0.129,-0.182]
[35.087,-0.0371,-0.0722,-0.103]
[43.865,-0.0184,-0.0359,-0.0518]
[54.841,-0.00899,-0.0176,-0.0255]
[68.563,-0.00467,-0.00915,-0.013]
[]
[]
[]
[null,"Wall deflection I1 (mm)",{"$nulls":6},"Wall deflection I1 (mm)"]
[null,null,"Computed ",{"$nulls":6},"Measured"]
["Elevation (m)","Stage 2","Stage4","Stage7",null,null,null,"Elevation(m)","Stage 2","Stage4","Stage7"]
[2.1,1.83,4.3,6.66,null,null,null,2.1,8.89,11.884,26.597]
[1.7952,1.77,4.3,6.68,null,null,null,1.7952,8.128,10.922,23.876]
[1.4904,1.72,4.3,6.69,null,null,null,1.4904,7.112,10.16,21.336]
[1.1856,1.66,4.3,6.7,null,null,null,1.1856,6.35,9.398,19.812]
[0.8808,1.59,4.28,6.7,null,null,null,0.8808,5.588,8.89,18.034]
[0.576,1.52,4.26,6.7,null,null,null,0.576,4.572,8.382,16.764]
[0.2712,1.45,4.22,6.68,null,null,null,0.2712,3.81,7.874,15.748]
[-0.0336,1.38,4.16,6.64,null,null,null,-0.0336,3.048,7.366,14.986]
[-0.3384,1.32,4.07,6.59,null,null,null,-0.3384,2.286,6.985,14.224]
[-0.6432,1.31,3.94,6.51,null,null,null,-0.6432,1.6002,6.604,13.462]
[-0.948,1.32,3.77,6.41,null,null,null,-0.948,1.016,6.096,12.7]
[-1.2528,1.34,3.56,6.28,null,null,null,-1.2528,0.762,5.588,11.938]
[-1.5576,1.36,3.31,6.12,null,null,null,-1.5576,0.508,5.08,11.176]
[-1.8624,1.38,3.05,5.95,null,null,null,-1.8624,0.254,4.572,10.668]
[-2.1672,1.38,2.77,5.76,null,null,null,-2.1672,null,3.937,10.16]
[-2.472,1.38,2.51,5.55,null,null,null,-2.472,null,3.429,9.652]
[-2.7768,1.38,2.28,5.4,null,null,null,-2.7768,null,2.921,9.144]
[-3.0816,1.38,2.23,5.22,null,null,null,-3.0816,null,2.413,8.382]
[-3.3864,1.38,2.24,5.01,null,null,null,-3.3864,null,1.778,7.874]
[-3.6912,1.37,2.28,4.76,null,null,null,-3.6912,null,1.27,7.366]
[-3.996,1.37,2.32,4.46,null,null,null,-3.996,null,0.762,6.858]
[-4.3008,1.36,2.36,4.13,null,null,null,-4.3008,null,0.508,6.35]
[-4.6056,1.35,2.39,3.76,null,null,null,-4.6056,null,0.254,5.588]
[-4.9104,1.34,2.41,3.38,null,null,null,-4.9104,null,null,4.826]
[-5.2152,1.32,2.42,3.01,null,null,null,-5.2152,null,null,4.064]
[-5.52,1.3,2.42,2.9,null,null,null,-5.52,null,null,3.302]
[-5.8248,1.29,2.41,2.87,null,null,null,-5.8248,null,null,2.54]
[-6.1296,1.27,2.41,2.88,null,null,null,-6.1296,null,null,2.032]
[-6.4344,1.25,2.4,2.9,null,null,null,-6.4344,null,null,1.524]
[-6.7392,1.24,2.4,2.94,null,null,null,-6.7392,null,null,1.27]
[-7.044,1.22,2.39,3.01,null,null,null,-7.044,null,null,1.016]
[-7.3488,1.17,2.31,2.94,null,null,null,-7.3488,null,null,0.762]
[-7.6536,1.14,2.26,2.88,null,null,null,-7.6536,null,null,0.508]
[-7.9584,1.11,2.2,2.83,null,null,null,-7.9584,null,null,0.254]
[-8.2632,1.07,2.15,2.77,null,null,null,-8.2632]
[-8.568,1.04,2.1,2.71,null,null,null,-8.568]
[-8.8728,1.01,2.04,2.64,null,null,null,-8.8728]
[-9.1776,0.978,1.98,2.57,null,null,null,-9.1776]
[-9.4824,0.945,1.92,2.5,null,null,null,-9.4824]
[-9.7872,0.911,1.86,2.42,null,null,null,-9.7872]
[-10.092,0.876,1.79,2.34,null,null,null,-10.092]
[-10.854,0.785,1.62,2.13,null,null,null,-10.854]
[-11.616,0.69,1.43,1.89,null,null,null,-11.616]
[-12.378,0.59,1.23,1.63,null,null,null,-12.378]
[-13.14,0.484,1.02,1.36,null,null,null,-13.14]
[-13.902,0.373,0.788,1.06,null,null,null,-13.902]
[-14.664,0.256,0.543,0.733,null,null,null,-14.664]
[-15.426,0.132,0.281,0.382,null,null,null,-15.426]
[-16.188,8.17e-31,7.93e-31,7.73e-31,null,null,null,-16.188]
[]
[]
[null,"I2 deflection (mm)",{"$nulls":6},"I2 deflection (mm)"]
[null,null,"Computed ",{"$nulls":6},"Measured"]
["Elevation (m)","Stage 2","Stage4","Stage7",null,null,null,"Elevation(m)","Stage 2","Stage4","Stage7"]
[2.1,0.99316,3.1828,5.5488,null,null,null,2.1,5.08,11.938,26.714]
[1.4904,1.1672,3.4265,5.7751,null,null,null,1.4904,3.9116,11.176,23.876]
[0.8808,1.2176,3.519,5.8711,null,null,null,0.8808,3.302,10.16,21.082]
[0.2712,1.2242,3.5095,5.8622,null,null,null,0.2712,2.794,9.144,18.542]
[-0.3384,1.2369,3.4156,5.7732,null,null,null,-0.3384,2.286,8.128,17.018]
[-0.948,1.2046,3.1481,5.6442,null,null,null,-0.948,1.778,7.112,15.494]
[-1.5576,1.2248,2.848,5.4075,null,null,null,-1.5576,1.2446,6.096,14.224]
[-2.1672,1.2422,2.5356,5.1047,null,null,null,-2.1672,0.8636,5.08,12.954]
[-2.7768,1.2399,2.2924,4.7692,null,null,null,-2.7768,0.508,3.81,11.684]
[-3.3864,1.2663,2.2738,4.5188,null,null,null,-3.3864,0.254,2.54,9.906]
[-3.996,1.2726,2.2077,3.9651,null,null,null,-3.996,null,1.778,8.382]
[-4.6056,1.2657,2.2296,3.4902,null,null,null,-4.6056,null,1.016,6.604]
[-5.2152,1.25,2.2519,3.1078,null,null,null,-5.2152,null,0.4572,4.826]
[-5.8248,1.23,2.2643,2.8938,null,null,null,-5.8248,null,0.254,3.302]
[-6.4344,1.2104,2.2664,2.8115,null,null,null,-6.4344,null,null,2.032]
[-7.044,1.1888,2.2495,2.77,null,null,null,-7.044,null,null,1.3138]
[-7.6536,1.1457,2.1862,2.6989,null,null,null,-7.6536,null,null,0.8382]
[-8.2632,1.0829,2.0883,2.6029,null,null,null,-8.2632,null,null,0.4572]
[-8.8728,1.0146,1.9782,2.4928,null,null,null,-8.8728,null,null,0.254]
[-9.4824,0.94515,1.861,2.3683,null,null,null,-9.4824]
[-10.092,0.874,1.736,2.2275,null,null,null,-10.092]
[-11.616,0.68652,1.3873,1.8074,null,null,null,-11.616]
[-13.14,0.4814,0.98512,1.2977,null,null,null,-13.14]
[-14.664,0.25436,0.52544,0.6987,null,null,null,-14.664]
[-16.188,9.3749e-33,1.0083e-32,4.1337e-33,null,null,null,-16.188]
[]
[]
[null,"I3 deflection (mm)",{"$nulls":6},"I3 deflection (mm)"]
[null,null,"Computed ",{"$nulls":6},"Measured"]
["Elevation (m)","Stage 2","Stage4","Stage7",null,null,null,"Elevation(m)","Stage 2","Stage4","Stage7"]
[2.1,0.547,1.93,3.99,null,null,null,2.1,0,6.35,14.732]
[1.4904,0.648,2.05,4.05,null,null,null,1.4904,0,5.842,13.208]
[0.8808,0.733,2.12,4.07,null,null,null,0.8808,0,5.334,11.684]
[0.2712,0.8,2.15,4.06,null,null,null,0.2712,0,4.953,10.414]
[-0.3384,0.854,2.16,4.02,null,null,null,-0.3384,0,4.572,9.398]
[-0.948,0.894,2.13,3.94,null,null,null,-0.948,0,4.064,8.636]
[-1.5576,0.928,2.08,3.8,null,null,null,-1.5576,0,3.556,7.62]
[-2.1672,0.958,2.02,3.63,null,null,null,-2.1672,0,3.048,6.35]
[-2.7768,0.975,1.95,3.42,null,null,null,-2.7768,0,2.54,5.08]
[-3.3864,1.01,1.93,3.29,null,null,null,-3.3864,0,2.032,3.81]
[-3.996,1.03,1.92,3.12,null,null,null,-3.996,0,1.524,2.54]
[-4.6056,1.04,1.92,2.97,null,null,null,-4.6056,0,1.016,1.778]
[-5.2152,1.04,1.93,2.83,null,null,null,-5.2152,0,0.762,1.27]
[-5.8248,1.04,1.92,2.7,null,null,null,-5.8248,0,0.254,0.762]
[-6.4344,1.03,1.91,2.58,null,null,null,-6.4344,0,0,0.254]
[-7.044,1.01,1.88,2.48,null,null,null,-7.044,0,0,0]
[-7.6536,0.98,1.84,2.37,null,null,null,-7.6536,0,0,0]
[-8.2632,0.943,1.78,2.27,null,null,null,-8.2632,0,0,0]
[-8.8728,0.898,1.7,2.16,null,null,null,-8.8728,0,0,0]
[-9.4824,0.847,1.62,2.05,null,null,null,-9.4824,0,0,0]
[-10.092,0.79,1.52,1.92,null,null,null,-10.092,0,0,0]
[-11.616,0.628,1.22,1.55,null,null,null,-11.616,0,0,0]
[-13.14,0.443,0.868,1.11,null,null,null,-13.14,0,0,0]
[-14.664,0.234,0.461,0.593,null,null,null,-14.664,0,0,0]
[-16.188,3.25e-32,3.19e-32,1.13e-32,null,null,null,-16.188,0,0,0]

{"sheet":"Figure 7","index":1,"n_rows":156,"n_cols":11,"rows_kept":156,"cut":false,"hidden":false,"merged":[[0,0,0,10]],"flags":["formulas_cached_only"]}
["FIG.7. Computed response, two anchor section, Texas A& M excavation, after six passes of SelfSim learning with wall deformations (I-1), lateral movements of inclinometer I-3, and tieback loads"]
[]
[{"$nulls":8},"Settlements (mm)"]
[null,"Settlements (mm)",{"$nulls":6},"Measured"]
[null,null,"Computed ",null,null,"Stage2",null,"Stage 4",null,"Stage 7"]
["Distance from the wall (m)","Stage 2","Stage 4","Stage 7",null,"Distance from the wall(m)","Settlemetns(mm)","Distance from the wall(m)","Settlemetns(mm)","Distance from the wall(m)","Settlemetns(mm)"]
[0,2.36,2.93,1.95,null,4.6604,-0.762,0.95402,3.3,0,21.8]
[0.0086868,2.35,2.93,1.97,null,7.9431,-1.65,4.6604,-1.78,1.8623,21.6]
[0.019568,2.34,2.93,1.99,null,9.7841,-1.93,7.9431,-3.3,4.6604,3.99]
[0.033162,2.33,2.93,2.02,null,14.966,0.254,9.7841,-3.05,7.9431,-3.81]
[0.049987,2.33,2.94,2.05,null,null,null,14.966,-0.508,9.7841,-1.24]
[0.071323,2.32,2.93,2.08,{"$nulls":5},14.966,-0.254]
[0.097841,2.3,2.91,2.08]
[0.13106,2.26,2.85,2.03]
[0.17252,2.2,2.75,1.92]
[0.22433,2.11,2.59,1.71]
[0.28926,1.97,2.37,1.47]
[0.36881,1.8,2.11,1.2]
[0.46939,1.58,1.83,0.935]
[0.59741,1.32,1.5,0.649]
[0.7559,1.05,1.14,0.36]
[0.95402,0.798,0.789,0.0756]
[1.2009,0.635,0.562,-0.114]
[1.4996,0.578,0.435,-0.236]
[1.8959,0.462,0.259,-0.354]
[2.3774,0.388,0.127,-0.449]
[2.9809,0.301,-0.0155,-0.517]
[3.7338,0.233,-0.0499,-0.436]
[4.6769,0.126,-0.138,-0.371]
[5.8564,0.0788,-0.128,-0.244]
[7.3286,0.0273,-0.164,-0.238]
[9.1696,0.00421,-0.126,-0.139]
[11.471,-0.0234,-0.154,-0.197]
[14.348,-0.0282,-0.12,-0.152]
[17.945,-0.0308,-0.107,-0.135]
[22.441,-0.0229,-0.0724,-0.0915]
[28.061,-0.0148,-0.0464,-0.0638]
[35.087,-0.00831,-0.0262,-0.0361]
[43.865,-0.00335,-0.0105,-0.0143]
[54.841,-0.00167,-0.00537,-0.00775]
[68.563,-0.000943,-0.00294,-0.00469]
[]
[]
[]
[null,"Wall deflection I1 (mm)",{"$nulls":6},"Wall deflection I1 (mm)"]
[null,null,"Computed ",{"$nulls":6},"Measured"]
["Elevation (m)","Stage 2","Stage4","Stage7",null,null,null,"Elevation(m)","Stage 2","Stage4","Stage7"]
[2.1,8.36,15.8,19,null,null,null,2.1,8.89,11.884,26.597]
[1.7952,7.62,14.9,18.1,null,null,null,1.7952,8.128,10.922,23.876]
[1.4904,6.89,14,17.3,null,null,null,1.4904,7.112,10.16,21.336]
[1.1856,6.16,13.1,16.5,null,null,null,1.1856,6.35,9.398,19.812]
[0.8808,5.43,12.2,15.7,null,null,null,0.8808,5.588,8.89,18.034]
[0.576,4.72,11.3,14.8,null,null,null,0.576,4.572,8.382,16.764]
[0.2712,4.03,10.5,14.1,null,null,null,0.2712,3.81,7.874,15.748]
[-0.0336,3.4,9.67,13.4,null,null,null,-0.0336,3.048,7.366,14.986]
[-0.3384,2.83,8.91,12.7,null,null,null,-0.3384,2.286,6.985,14.224]
[-0.6432,2.36,8.18,12.1,null,null,null,-0.6432,1.6002,6.604,13.462]
[-0.948,1.99,7.47,11.5,null,null,null,-0.948,1.016,6.096,12.7]
[-1.2528,1.7,6.77,11,null,null,null,-1.2528,0.762,5.588,11.938]
[-1.5576,1.47,6.08,10.5,null,null,null,-1.5576,0.508,5.08,11.176]
[-1.8624,1.3,5.41,9.99,null,null,null,-1.8624,0.254,4.572,10.668]
[-2.1672,1.16,4.77,9.52,null,null,null,-2.1672,null,3.937,10.16]
[-2.472,1.07,4.17,9.07,null,null,null,-2.472,null,3.429,9.652]
[-2.7768,1.01,3.64,8.7,null,null,null,-2.7768,null,2.921,9.144]
[-3.0816,0.979,3.27,8.33,null,null,null,-3.0816,null,2.413,8.382]
[-3.3864,0.966,2.98,7.91,null,null,null,-3.3864,null,1.778,7.874]
[-3.6912,0.961,2.76,7.42,null,null,null,-3.6912,null,1.27,7.366]
[-3.996,0.957,2.6,6.85,null,null,null,-3.996,null,0.762,6.858]
[-4.3008,0.948,2.47,6.2,null,null,null,-4.3008,null,0.508,6.35]
[-4.6056,0.934,2.36,5.49,null,null,null,-4.6056,null,0.254,5.588]
[-4.9104,0.912,2.25,4.77,null,null,null,-4.9104,null,null,4.826]
[-5.2152,0.883,2.15,4.07,null,null,null,-5.2152,null,null,4.064]
[-5.52,0.848,2.05,3.56,null,null,null,-5.52,null,null,3.302]
[-5.8248,0.809,1.94,3.15,null,null,null,-5.8248,null,null,2.54]
[-6.1296,0.768,1.84,2.84,null,null,null,-6.1296,null,null,2.032]
[-6.4344,0.728,1.75,2.61,null,null,null,-6.4344,null,null,1.524]
[-6.7392,0.693,1.66,2.43,null,null,null,-6.7392,null,null,1.27]
[-7.044,0.658,1.6,2.33,null,null,null,-7.044,null,null,1.016]
[-7.3488,0.524,1.33,2.02,null,null,null,-7.3488,null,null,0.762]
[-7.6536,0.418,1.08,1.65,null,null,null,-7.6536,null,null,0.508]
[-7.9584,0.314,0.828,1.27,null,null,null,-7.9584,null,null,0.254]
[-8.2632,0.216,0.583,0.879,null,null,null,-8.2632]
[-8.568,0.119,0.335,0.463,null,null,null,-8.568]
[-8.8728,0.0225,0.0812,0.0124,null,null,null,-8.8728]
[-9.1776,0.0509,0.13,0.0942,null,null,null,-9.1776]
[-9.4824,0.0754,0.174,0.167,null,null,null,-9.4824]
[-9.7872,0.0949,0.211,0.221,null,null,null,-9.7872]
[-10.092,0.11,0.24,0.26,null,null,null,-10.092]
[-10.854,0.133,0.288,0.318,null,null,null,-10.854]
[-11.616,0.143,0.309,0.34,null,null,null,-11.616]
[-12.378,0.14,0.303,0.39,null,null,null,-12.378]
[-13.14,0.127,0.274,0.444,null,null,null,-13.14]
[-13.902,0.107,0.229,0.399,null,null,null,-13.902]
[-14.664,0.0796,0.172,0.265,null,null,null,-14.664]
[-15.426,0.045,0.101,0.103,null,null,null,-15.426]
[-16.188,-7.94e-31,-7.6e-31,-7.01e-31,null,null,null,-16.188]
[]
[]
[null,"I2 deflection (mm)",{"$nulls":6},"I2 deflection (mm)"]
[null,null,"Computed ",{"$nulls":6},"Measured"]
["Elevation (m)","Stage 2","Stage4","Stage7",null,null,null,"Elevation(m)","Stage 2","Stage4","Stage7"]
[2.1,6.4287,13.45,17.018,null,null,null,2.1,5.08,11.938,26.714]
[1.4904,5.1723,11.725,15.279,null,null,null,1.4904,3.9116,11.176,23.876]
[0.8808,3.8139,9.9039,13.532,null,null,null,0.8808,3.302,10.16,21.082]
[0.2712,2.8987,8.4993,12.094,null,null,null,0.2712,2.794,9.144,18.542]
[-0.3384,2.7638,8.1738,11.693,null,null,null,-0.3384,2.286,8.128,17.018]
[-0.948,1.9718,6.9244,10.709,null,null,null,-0.948,1.778,7.112,15.494]
[-1.5576,1.4942,5.6788,9.6538,null,null,null,-1.5576,1.2446,6.096,14.224]
[-2.1672,1.1781,4.509,8.6189,null,null,null,-2.1672,0.8636,5.08,12.954]
[-2.7768,0.91433,3.4481,7.4685,null,null,null,-2.7768,0.508,3.81,11.684]
[-3.3864,0.84864,3.1184,6.7102,null,null,null,-3.3864,0.254,2.54,9.906]
[-3.996,0.86264,2.5935,5.6647,null,null,null,-3.996,null,1.778,8.382]
[-4.6056,0.81304,2.1979,4.6489,null,null,null,-4.6056,null,1.016,6.604]
[-5.2152,0.75811,1.9007,3.7103,null,null,null,-5.2152,null,0.4572,4.826]
[-5.8248,0.70677,1.6822,2.951,null,null,null,-5.8248,null,0.254,3.302]
[-6.4344,0.64875,1.485,2.3314,null,null,null,-6.4344,null,null,2.032]
[-7.044,0.55148,1.2297,1.7669,null,null,null,-7.044,null,null,1.3138]
[-7.6536,0.3969,0.88327,1.2273,null,null,null,-7.6536,null,null,0.8382]
[-8.2632,0.29562,0.65264,0.87103,null,null,null,-8.2632,null,null,0.4572]
[-8.8728,0.14008,0.33045,0.46404,null,null,null,-8.8728,null,null,0.254]
[-9.4824,0.15885,0.34554,0.50584,null,null,null,-9.4824]
[-10.092,0.15917,0.33149,0.58506,null,null,null,-10.092]
[-11.616,0.15565,0.33008,0.33539,null,null,null,-11.616]
[-13.14,0.13725,0.30267,0.21141,null,null,null,-13.14]
[-14.664,0.085118,0.17509,0.29384,null,null,null,-14.664]
[-16.188,-1.7784e-33,-7.5827e-33,-1.2689e-31,null,null,null,-16.188]
[]
[]
[null,"I3 deflection (mm)",{"$nulls":6},"I3 deflection (mm)"]
[null,null,"Computed ",{"$nulls":6},"Measured"]
["Elevation (m)","Stage 2","Stage4","Stage7",null,null,null,"Elevation(m)","Stage 2","Stage4","Stage7"]
[2.1,3.48,9.29,13.3,null,null,null,2.1,0,6.35,14.732]
[1.4904,2.79,7.9,11.7,null,null,null,1.4904,0,5.842,13.208]
[0.8808,2.22,6.9,10.6,null,null,null,0.8808,0,5.334,11.684]
[0.2712,1.8,5.88,8.85,null,null,null,0.2712,0,4.953,10.414]
[-0.3384,1.7,5.59,8.52,null,null,null,-0.3384,0,4.572,9.398]
[-0.948,1.46,5.02,7.92,null,null,null,-0.948,0,4.064,8.636]
[-1.5576,1.18,4.26,7.09,null,null,null,-1.5576,0,3.556,7.62]
[-2.1672,0.955,3.44,6.09,null,null,null,-2.1672,0,3.048,6.35]
[-2.7768,0.73,2.58,4.85,null,null,null,-2.7768,0,2.54,5.08]
[-3.3864,0.62,2.1,4,null,null,null,-3.3864,0,2.032,3.81]
[-3.996,0.504,1.63,3.16,null,null,null,-3.996,0,1.524,2.54]
[-4.6056,0.383,1.18,2.32,null,null,null,-4.6056,0,1.016,1.778]
[-5.2152,0.364,1.08,2.04,null,null,null,-5.2152,0,0.762,1.27]
[-5.8248,0.338,0.967,1.73,null,null,null,-5.8248,0,0.254,0.762]
[-6.4344,0.308,0.854,1.44,null,null,null,-6.4344,0,0,0.254]
[-7.044,0.276,0.744,1.19,null,null,null,-7.044,0,0,0]
[-7.6536,0.247,0.643,0.991,null,null,null,-7.6536,0,0,0]
[-8.2632,0.221,0.555,0.862,null,null,null,-8.2632,0,0,0]
[-8.8728,0.201,0.483,0.777,null,null,null,-8.8728,0,0,0]
[-9.4824,0.187,0.428,0.712,null,null,null,-9.4824,0,0,0]
[-10.092,0.175,0.385,0.65,null,null,null,-10.092,0,0,0]
[-11.616,0.15,0.314,0.462,null,null,null,-11.616,0,0,0]
[-13.14,0.118,0.246,0.304,null,null,null,-13.14,0,0,0]
[-14.664,0.0694,0.145,0.174,null,null,null,-14.664,0,0,0]
[-16.188,-1.79e-34,3.03e-33,6.96e-33,null,null,null,-16.188,0,0,0]

{"sheet":"Figure 8","index":2,"n_rows":10,"n_cols":11,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,12]],"flags":["formulas_cached_only"]}
["FIG.8. Comparison of measured and computed tieback loads in two-level tieback section of the wall, Texas A&M excavation"]
[]
["Anchor 1",{"$nulls":5},"Anchor 2"]
[]
[null,"Tie back (kN)",{"$nulls":5},"Tie back (kN)"]
[null,"Computed",null,null,"Measured",null,null,"Computed",null,null,"Measured"]
["Excavation depth (m)","Wall only","Wall+I3","Wall+I3+RF",null,null,"Excavation depth (m)","Wall only","Wall+I3","Wall+I3+RF"]
[4.6,476,412,392,373,null,7.5,540,486,324,293]
[6.3,468,454,402,381]
[7.5,422,414,366,377]

{"sheet":"Figure 10","index":3,"n_rows":160,"n_cols":9,"rows_kept":160,"cut":false,"hidden":false,"merged":[[0,0,1,10]],"flags":["formulas_cached_only"]}
["FIG.10. Predicted excavation response in single tieback level section, Texas A& M excavation,  using developed model from learning wall deflections (I-1), lateral movements of inclinometer I-3 and tieback loads in two-level tieback section of the wall"]
[]
[]
[null,"Settlements (mm)",{"$nulls":4},"Settlements (mm)"]
[null,null,"Predicted ",null,null,null,"Measured"]
["Distance from the wall (m)","Stage 2","Stage3","Stage6",null,"Distance from the wall(m)","Stage 2","Stage3","Stage6"]
[0,2.18,2.14,2.51,null,0,null,null,11.176]
[0.0086868,2.18,2.15,2.52,null,0.95402,null,-0.508]
[0.019568,2.17,2.15,2.53,null,1.8623,null,null,8.382]
[0.033162,2.17,2.15,2.53]
[0.049987,2.17,2.15,2.54,null,4.6604,-1.3511,-1.016,2.794]
[0.071323,2.17,2.16,2.55]
[0.097841,2.16,2.16,2.57,null,7.9431,-1.3462,-2.794,1.27]
[0.13106,2.15,2.15,2.58]
[0.17252,2.14,2.15,2.58,null,9.7841,-2.0574,-0.762]
[0.22433,2.11,2.13,2.59,null,14.966,0.254,-0.254,0]
[0.28926,2.07,2.09,2.54,null,18.562,null,null,0]
[0.36881,2,2.03,2.44]
[0.46939,1.89,1.93,2.29]
[0.59741,1.75,1.78,2.09]
[0.7559,1.56,1.6,1.88]
[0.95402,1.33,1.36,1.55]
[1.2009,1.11,1.15,1.28]
[1.4996,0.995,1.03,1.17]
[1.8959,0.862,0.899,1.02]
[2.3774,0.736,0.769,0.855]
[2.9809,0.58,0.61,0.621]
[3.7338,0.42,0.445,0.381]
[4.6769,0.223,0.244,0.0828]
[5.8564,0.0733,0.0894,-0.127]
[7.3286,-0.0372,-0.0234,-0.315]
[9.1696,-0.0958,-0.0839,-0.381]
[11.471,-0.121,-0.11,-0.411]
[14.348,-0.112,-0.101,-0.352]
[17.945,-0.0959,-0.0855,-0.297]
[22.441,-0.0676,-0.059,-0.21]
[28.061,-0.0458,-0.0393,-0.144]
[35.087,-0.0265,-0.0225,-0.0845]
[43.865,-0.0133,-0.0113,-0.0428]
[54.841,-0.0066,-0.00569,-0.0215]
[68.563,-0.00367,-0.00336,-0.0129]
[]
[]
[]
[]
[null,"Wall deflection I4 (mm)",{"$nulls":4},"Wall deflection I4 (mm)"]
[null,null,"Predicted ",{"$nulls":4},"Measured"]
["Elevation (m)","Stage 2","Stage3","Stage6",null,"Elevation(m)","Stage 2","Stage3","Stage6"]
[2.1,6.19,5.66,12.2,null,2.1,8.89,11.884,17.018]
[1.7952,5.8,5.27,11.8,null,1.7952,8.128,10.922,16.256]
[1.4904,5.4,4.89,11.3,null,1.4904,7.62,10.16,15.24]
[1.1856,5,4.5,10.9,null,1.1856,6.858,9.398,13.97]
[0.8808,4.61,4.11,10.5,null,0.8808,6.096,8.128,12.7]
[0.576,4.21,3.73,10.1,null,0.576,5.588,7.112,11.684]
[0.2712,3.83,3.36,9.65,null,0.2712,4.826,6.096,10.922]
[-0.0336,3.45,2.99,9.24,null,-0.0336,4.064,4.826,10.414]
[-0.3384,3.08,2.64,8.85,null,-0.3384,3.556,3.556,9.906]
[-0.6432,2.74,2.31,8.48,null,-0.6432,2.794,2.286,9.652]
[-0.948,2.41,2,8.11,null,-0.948,2.54,1.27,9.398]
[-1.2528,2.12,1.73,7.79,null,-1.2528,2.032,0.762,9.144]
[-1.5576,1.86,1.5,7.47,null,-1.5576,1.524,0.254,8.89]
[-1.8624,1.63,1.3,7.16,null,-1.8624,1.016,0,8.636]
[-2.1672,1.44,1.14,6.84,null,-2.1672,0.762,0,8.382]
[-2.472,1.28,1.01,6.51,null,-2.472,0.508,0,7.874]
[-2.7768,1.15,0.901,6.16,null,-2.7768,0.254,0,7.366]
[-3.0816,1.05,0.823,5.79,null,-3.0816,0,0,7.112]
[-3.3864,0.966,0.763,5.39,null,-3.3864,0,0,6.604]
[-3.6912,0.9,0.716,4.97,null,-3.6912,0,0,6.096]
[-3.996,0.846,0.679,4.53,null,-3.996,0,0,5.588]
[-4.3008,0.799,0.649,4.07,null,-4.3008,0,0,5.08]
[-4.6056,0.757,0.621,3.61,null,-4.6056,0,0,4.572]
[-4.9104,0.719,0.596,3.14,null,-4.9104,0,0,4.064]
[-5.2152,0.683,0.571,2.7,null,-5.2152,0,0,3.556]
[-5.52,0.647,0.546,2.3,null,-5.52,0,0,3.048]
[-5.8248,0.613,0.521,1.94,null,-5.8248,0,0,2.54]
[-6.1296,0.579,0.496,1.64,null,-6.1296,0,0,2.032]
[-6.4344,0.547,0.472,1.38,null,-6.4344,0,0,1.524]
[-6.7392,0.517,0.45,1.16,null,-6.7392,0,0,1.016]
[-7.044,0.486,0.426,0.962,null,-7.044,0,0,0.508]
[-7.3488,0.374,0.319,0.818,null,-7.3488,0,0,0.254]
[-7.6536,0.303,0.252,0.659,null,-7.6536,0,0,0]
[-7.9584,0.23,0.183,0.486,null,-7.9584,0,0,0]
[-8.2632,0.16,0.117,0.304,null,-8.2632,0,0,0]
[-8.568,0.0907,0.0513,0.105,null,-8.568,0,0,0]
[-8.8728,0.0232,-0.0128,-0.128,null,-8.8728,0,0,0]
[-9.1776,0.0549,0.0218,-0.0364,null,-9.1776,0,0,0]
[-9.4824,0.0838,0.0534,0.0485,null,-9.4824,0,0,0]
[-9.7872,0.108,0.0804,0.122,null,-9.7872,0,0,0]
[-10.092,0.129,0.103,0.185,null,-10.092,0,0,0]
[-10.854,0.164,0.144,0.303,null,-10.854,0,0,0]
[-11.616,0.181,0.166,0.371,null,-11.616,0,0,0]
[-12.378,0.183,0.172,0.397,null,-12.378,0,0,0]
[-13.14,0.172,0.164,0.387,null,-13.14,0,0,0]
[-13.902,0.148,0.143,0.343,null,-13.902,0,0,0]
[-14.664,0.112,0.109,0.266,null,-14.664,0,0,0]
[-15.426,0.0627,0.0614,0.153,null,-15.426,0,0,0]
[-16.188,8.15e-31,8.15e-31,7.95e-31,null,-16.188,0,0,0]
[]
[]
[]
[]
[null,"I5 deflection (mm)",{"$nulls":4},"I5 deflection (mm)"]
[null,null,"Computed ",{"$nulls":4},"Measured"]
["Elevation (m)","Stage 2","Stage3","Stage6",null,"Elevation(m)","Stage 2","Stage3","Stage6"]
[2.1,4.8,4.4,11,null,2.1,5.08,6.35,11.938]
[1.4904,4.22,3.8,10.1,null,1.4904,3.9116,5.08,10.922]
[0.8808,3.48,3.06,9.1,null,0.8808,3.302,3.81,10.16]
[0.2712,2.66,2.25,7.78,null,0.2712,2.794,2.54,9.144]
[-0.3384,2.7,2.31,7.91,null,-0.3384,2.286,1.016,8.382]
[-0.948,2.15,1.79,7.38,null,-0.948,1.778,0.254,7.62]
[-1.5576,1.73,1.41,6.88,null,-1.5576,1.2446,0,7.112]
[-2.1672,1.39,1.1,6.39,null,-2.1672,0.8636,0,6.858]
[-2.7768,1.13,0.879,5.65,null,-2.7768,0.508,0,6.604]
[-3.3864,1.1,0.894,5.18,null,-3.3864,0.254,0,6.096]
[-3.996,0.953,0.788,4.33,null,-3.996,0,0,5.334]
[-4.6056,0.86,0.725,3.58,null,-4.6056,0,0,4.572]
[-5.2152,0.788,0.677,2.87,null,-5.2152,0,0,3.81]
[-5.8248,0.728,0.635,2.22,null,-5.8248,0,0,3.048]
[-6.4344,0.67,0.593,1.68,null,-6.4344,0,0,2.286]
[-7.044,0.603,0.538,1.24,null,-7.044,0,0,1.524]
[-7.6536,0.489,0.434,0.874,null,-7.6536,0,0,0.762]
[-8.2632,0.325,0.278,0.533,null,-8.2632,0,0,0.254]
[-8.8728,0.133,0.093,0.183,null,-8.8728,0,0,0]
[-9.4824,0.17,0.137,0.252,null,-9.4824,0,0,0]
[-10.092,0.194,0.166,0.32,null,-10.092,0,0,0]
[-11.616,0.214,0.197,0.423,null,-11.616,0,0,0]
[-13.14,0.188,0.179,0.404,null,-13.14,0,0,0]
[-14.664,0.118,0.114,0.266,null,-14.664,0,0,0]
[-16.188,-1.19e-34,-4.45e-34,-1.54e-34,null,-16.188,0,0,0]
[]
[]
[]
[null,"I6 deflection (mm)",{"$nulls":4},"I6 deflection (mm)"]
[null,null,"Computed ",{"$nulls":4},"Measured"]
["Elevation (m)","Stage 2","Stage3","Stage6",null,"Elevation(m)","Stage 2","Stage3","Stage6"]
[2.1,2.57,2.31,8.12,null,2.1,0,0,7.112]
[1.4904,2.29,2.02,7.22,null,1.4904,0,0,6.604]
[0.8808,1.91,1.65,6.27,null,0.8808,0,0,6.35]
[0.2712,1.54,1.27,5.4,null,0.2712,0,0,5.842]
[-0.3384,1.59,1.34,5.56,null,-0.3384,0,0,5.334]
[-0.948,1.49,1.25,5.46,null,-0.948,0,0,4.826]
[-1.5576,1.32,1.1,5.22,null,-1.5576,0,0,4.572]
[-2.1672,1.17,0.964,4.91,null,-2.1672,0,0,4.318]
[-2.7768,1.02,0.834,4.43,null,-2.7768,0,0,4.064]
[-3.3864,0.983,0.815,4.08,null,-3.3864,0,0,3.556]
[-3.996,0.931,0.786,3.67,null,-3.996,0,0,3.048]
[-4.6056,0.873,0.747,3.23,null,-4.6056,0,0,2.794]
[-5.2152,0.817,0.707,2.81,null,-5.2152,0,0,2.286]
[-5.8248,0.753,0.658,2.39,null,-5.8248,0,0,1.778]
[-6.4344,0.681,0.599,1.98,null,-6.4344,0,0,1.27]
[-7.044,0.598,0.527,1.59,null,-7.044,0,0,0.762]
[-7.6536,0.499,0.438,1.22,null,-7.6536,0,0,0.254]
[-8.2632,0.382,0.33,0.867,null,-8.2632,0,0,0]
[-8.8728,0.244,0.199,0.529,null,-8.8728,0,0,0]
[-9.4824,0.241,0.203,0.502,null,-9.4824,0,0,0]
[-10.092,0.24,0.207,0.487,null,-10.092,0,0,0]
[-11.616,0.224,0.203,0.451,null,-11.616,0,0,0]
[-13.14,0.183,0.171,0.373,null,-13.14,0,0,0]
[-14.664,0.109,0.104,0.225,null,-14.664,0,0,0]
[-16.188,-5.33e-34,-2.9e-33,-7.13e-34,null,-16.188,0,0,0]

{"sheet":"Figure 11","index":4,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,12]],"flags":["formulas_cached_only"]}
["FIG.11. Comparison of measured and predicted tieback loads in single tieback level section of the wall, Texas A&M excavation"]
[]
["Anchor"]
[]
[null,"Tie back (kN)"]
[null,"Computed",null,null,"Measured"]
["Excavation depth (m)","Wall only","Wall+I3","Wall+I3+RF"]
[4.2,430,380,337.5,304.14]
[6.3,410,430,378,310.8]
[7.5,520,460,440.5,326.34]

{"sheet":"Figure 15","index":5,"n_rows":86,"n_cols":18,"rows_kept":86,"cut":false,"hidden":false,"merged":[[0,0,0,15]],"flags":["formulas_cached_only"]}
["FIG.15. Original  and target measurements for inverse analysis for a) lateral wall deflections of I05 & I06, and b) surface settlements CJ04, Shanghai excavation"]
[]
[{"$nulls":7},"I05",{"$nulls":5},"I06"]
["Proposed measurement",{"$nulls":6},"Measured",{"$nulls":5},"Measured"]
["Wall defelction (mm)",{"$nulls":6},"Wall defelction (mm)",{"$nulls":5},"Wall defelction (mm)"]
["Elevation(m)","Stage 2","Stage 3","Stage 4","Stage 5",null,"Elevation(m)","Stage 2","Stage 3","Stage 4","Stage 5",null,null,"Elevation(m)","Stage 2","Stage 3","Stage 4","Stage 5"]
[0,0.4,0.4,0.4,0.4,null,0,null,-0.54,-0.61,-1.59,null,null,0,null,0.92,0.43,0.54]
[0.5,0.5,0.5,0.5,0.5,null,1,-0.18,-0.35,-0.12,-0.88,null,null,1,null,1.12,1.06,1.26]
[1,0.7,0.7,0.7,0.7,null,2,-0.32,-0.23,-0.01,-0.14,null,null,2,null,1.37,1.39,1.84]
[1.5,0.9,0.9,0.9,0.9,null,3,-0.37,null,0.33,0.46,null,null,3,null,1.6,1.84,2.32]
[2,1.1,1.1,1.1,1.1,null,4,-0.29,0.51,1.01,1.45,null,null,4,null,2.1,2.75,3.34]
[2.5,1.4,1.4,1.4,1.4,null,5,0.04,1.14,2.04,2.67,null,null,5,null,2.67,3.77,4.35]
[3,1.6,1.6,1.6,1.6,null,6,0.67,2.25,3.63,4.67,null,null,6,null,3.32,4.85,5.53]
[3.5,1.9,1.9,1.9,1.9,null,7,1.35,3.45,5.48,7.05,null,null,7,null,3.86,5.81,6.72]
[4,2.3,2.3,2.3,2.3,null,8,1.83,4.49,7.24,9.14,null,null,8,null,4.48,6.94,8.2]
[4.5,2.7,2.7,2.7,2.7,null,9,1.9,5.18,8.69,10.98,null,null,9,null,4.9,7.88,9.99]
[5,3.2,3.2,3.2,3.2,null,10,1.86,5.7,9.97,12.77,null,null,10,null,5.25,8.79,11.5]
[5.5,3.5,3.9,3.9,3.9,null,11,1.83,6.08,11.07,14.69,null,null,11,null,5.56,9.54,13.06]
[6,3.8,4.7,4.7,4.7,null,12,1.68,6.18,11.53,16.11,null,null,12,null,5.54,9.94,14.49]
[6.5,3.9,5.6,5.6,5.6,null,13,1.19,5.8,11.45,17.07,null,null,13,null,5.55,10.31,15.71]
[7,3.8,6.6,6.6,6.6,null,14,0.64,5.26,10.98,17.55,null,null,14,null,5.5,10.36,16.66]
[7.5,3.7,7.2,7.4,7.4,null,15,0.89,5.55,11.36,18.58,null,null,15,null,5.36,10.33,17.49]
[8,3.5,7.8,8.4,8.4,null,16,0.85,5.33,11.01,18.79,null,null,16,null,5.09,10.02,17.68]
[8.5,3.3,8,9.4,9.4,null,17,0.61,4.81,10.39,18.58,null,null,17,null,4.84,9.68,17.59]
[9,3.2,8.2,10.2,10.2,null,18,0.5,4.34,9.32,17.67,null,null,18,null,4.51,9.15,17.23]
[9.5,3,8.3,11,11,null,19,0.53,3.96,8.38,16.53,null,null,19,null,4.06,8.39,16.38]
[10,2.9,8.2,11.8,11.9,null,20,0.46,3.66,7.71,15.67,null,null,20,null,3.55,7.67,15.4]
[10.5,2.7,8.1,12.2,12.8,null,21,0.43,3.29,7.03,14.3,null,null,21,null,3.1,6.97,14.36]
[11,2.6,7.8,12.7,14,null,22,0.39,2.89,5.98,12.67,null,null,22,null,2.79,6.3,13.28]
[11.5,2.4,7.6,13,15,null,23,0.35,2.39,5.14,11.17,null,null,23,null,2.51,5.5,11.95]
[12,2.2,7.3,13.1,16.4,null,24,0.11,1.85,4.65,9.97,null,null,24,null,2.16,4.61,10.18]
[12.5,2,7.1,13.2,17.2,null,25,-1.1102e-16,1.81,4.41,9.09,null,null,25,null,1.82,3.99,8.99]
[13,1.8,6.8,13.1,17.7,null,26,0.03,1.65,3.8,8.14,null,null,26,null,1.4,3.29,7.88]
[13.5,1.6,6.6,12.9,18,null,27,0.04,1.45,3.34,7.33,null,null,27,null,1.35,3.18,7.42]
[14,1.4,6.4,12.7,18.1]
[14.5,1.3,6.1,12.3,18.2]
[15,1.2,5.9,11.9,18]
[15.5,1,5.7,11.5,17.7]
[16,0.9,5.5,11.1,17.4]
[16.5,0.8,5.3,10.7,17]
[17,0.7,5.1,10.3,16.6]
[17.5,0.6,4.9,9.9,16.2]
[18,0.5,4.7,9.5,15.7]
[18.5,0.4,4.5,9.1,15.2]
[19,0.35,4.3,8.8,14.8]
[19.5,0.3,4.1,8.4,14.3]
[20,0.25,3.9,8,13.8]
[20.5,0.2,3.7,7.6,13.3]
[21,0.1,3.5,7.3,12.8]
[21.5,0.05,3.3,6.9,12.3]
[22,0.03,3.1,6.5,11.8]
[22.5,0.01,2.9,6.3,11.3]
[23,null,2.7,5.9,10.8]
[23.5,null,2.5,5.5,10.3]
[24,null,2.3,5.2,9.8]
[24.5,null,2.1,4.8,9.4]
[25,null,1.9,4.4,8.9]
[25.5,null,1.7,4.2,8.4]
[26,null,1.5,3.9,7.9]
[26.5,null,1.4,3.7,7.4]
[27,null,1.3,3.4,7]
{"$rows_empty":7}
["Proposed measurements",{"$nulls":6},"CJ04"]
["Settlements(mm)",{"$nulls":6},"Measured"]
["Distance from the wall (m)","Stage 2","Stage 3","Stage 4","Stage 5",null,"Stage 2",null,"Stage 3",null,"Stage 4",null,"Stage 5"]
[0,{"$nulls":5},"Distance from the wall (m)","Settlements(mm)","Distance from the wall (m)","Settlements(mm)","Distance from the wall (m)","Settlements(mm)","Distance from the wall (m)","Settlements(mm)"]
[1.012,0.5,1,1.7,null,null,1.9751,1.0008,1.9751,1.4756,2.0078,2.81,1.9751,3.2719]
[2.077,1.2,1.8,2.9,3.5,null,5.0032,2.0017,5.0032,2.6689,4.9378,5.2736,4.9705,6.082]
[3.1984,1.4,2.1,3.9,4.5,null,8.9926,1.8733,9.058,2.5406,8.9926,4.94,9.0253,6.685]
[4.3788,1.8,2.4,4.6,5.8,null,13.996,1.0008,14.035,1.4756,14.035,2.9383,14.068,4.0803]
[5.6213,1.9,2.6,5,6.3,null,20.13,0.87252,20.13,1.142,20.13,2.3994,20.098,3.2719]
[6.9292,2,2.7,5.3,6.6]
[8.306,1.95,2.65,5.35,6.6]
[9.7553,1.85,2.5,5,6.25]
[11.281,1.7,2.3,4.5,5.7]
[12.887,1.45,2,3.9,5.1]
[14.577,1.3,1.8,3.4,4.5]
[16.356,1.15,1.5,2.85,4]
[18.229,1,1.3,2.4,3.4]
[20.201,0.7,1,1.95,2.9]

{"sheet":"Figure 16","index":6,"n_rows":115,"n_cols":11,"rows_kept":115,"cut":false,"hidden":false,"merged":[[0,0,0,12]],"flags":["formulas_cached_only"]}
["FIG.16. Computed deformations in Cluster 1 prior to SelfSim learning; a) wall deformations, and b) surface settlements, Shanghai excavation"]
[]
[null,"Wall deflection (mm)",{"$nulls":6},"Wall deflection (mm)"]
[null,null,"SelfSim",{"$nulls":5},"Proposed measurements"]
["Elevation (m)","Stage 2","Stage3","Stage4","Stage5",null,"Elevation (m)","Stage 2","Stage3","Stage4","Stage5"]
[0,0.485,0.482,0.495,0.493,null,0,0.4,0.4,0.4,0.4]
[0.5,0.602,0.594,0.6,0.601,null,0.5,0.5,0.5,0.5,0.5]
[1,0.72,0.707,0.706,0.709,null,1,0.7,0.7,0.7,0.7]
[1.5,0.84,0.822,0.814,0.819,null,1.5,0.9,0.9,0.9,0.9]
[2,0.951,0.93,0.914,0.921,null,2,1.1,1.1,1.1,1.1]
[2.5,1.05,1.03,1,1.01,null,2.5,1.4,1.4,1.4,1.4]
[3,1.13,1.1,1.07,1.08,null,3,1.6,1.6,1.6,1.6]
[3.5,1.18,1.17,1.13,1.14,null,3.5,1.9,1.9,1.9,1.9]
[4,1.22,1.22,1.18,1.18,null,4,2.3,2.3,2.3,2.3]
[4.5,1.24,1.28,1.23,1.23,null,4.5,2.7,2.7,2.7,2.7]
[5,1.25,1.35,1.29,1.28,null,5,3.2,3.2,3.2,3.2]
[5.5,1.24,1.41,1.37,1.34,null,5.5,3.5,3.9,3.9,3.9]
[6,1.23,1.46,1.45,1.41,null,6,3.8,4.7,4.7,4.7]
[6.5,1.21,1.5,1.54,1.48,null,6.5,3.9,5.6,5.6,5.6]
[7,1.18,1.52,1.66,1.57,null,7,3.8,6.6,6.6,6.6]
[7.5,1.15,1.53,1.78,1.66,null,7.5,3.7,7.2,7.4,7.4]
[8,1.12,1.53,1.88,1.74,null,8,3.5,7.8,8.4,8.4]
[8.5,1.08,1.52,1.95,1.8,null,8.5,3.3,8,9.4,9.4]
[9,1.04,1.51,1.98,1.85,null,9,3.2,8.2,10.2,10.2]
[9.5,1.01,1.49,1.97,1.91,null,9.5,3,8.3,11,11]
[10,0.971,1.47,1.95,2.01,null,10,2.9,8.2,11.8,11.9]
[10.5,0.935,1.44,1.92,2.12,null,10.5,2.7,8.1,12.2,12.8]
[11,0.899,1.4,1.89,2.21,null,11,2.6,7.8,12.7,14]
[11.5,0.865,1.37,1.87,2.25,null,11.5,2.4,7.6,13,15]
[12,0.831,1.33,1.84,2.26,null,12,2.2,7.3,13.1,16.4]
[12.5,0.8,1.29,1.81,2.23,null,12.5,2,7.1,13.2,17.2]
[13,0.769,1.25,1.77,2.19,null,13,1.8,6.8,13.1,17.7]
[13.5,0.739,1.21,1.74,2.15,null,13.5,1.6,6.6,12.9,18]
[14,0.711,1.18,1.7,2.11,null,14,1.4,6.4,12.7,18.1]
[14.5,0.684,1.14,1.66,2.08,null,14.5,1.3,6.1,12.3,18.2]
[15,0.658,1.1,1.62,2.05,null,15,1.2,5.9,11.9,18]
[15.5,0.634,1.07,1.57,2.02,null,15.5,1,5.7,11.5,17.7]
[16,0.611,1.03,1.53,1.98,null,16,0.9,5.5,11.1,17.4]
[16.5,0.589,0.997,1.49,1.95,null,16.5,0.8,5.3,10.7,17]
[17,0.568,0.964,1.45,1.91,null,17,0.7,5.1,10.3,16.6]
[17.5,0.548,0.934,1.41,1.87,null,17.5,0.6,4.9,9.9,16.2]
[18,0.529,0.903,1.36,1.83,null,18,0.5,4.7,9.5,15.7]
[18.5,0.511,0.875,1.32,1.78,null,18.5,0.4,4.5,9.1,15.2]
[19,0.494,0.847,1.28,1.74,null,19,0.35,4.3,8.8,14.8]
[19.5,0.478,0.821,1.25,1.69,null,19.5,0.3,4.1,8.4,14.3]
[20.5,0.448,0.771,1.17,1.61,null,20,0.25,3.9,8,13.8]
[21.5,0.421,0.725,1.1,1.52,null,20.5,0.2,3.7,7.6,13.3]
[22.5,0.397,0.683,1.04,1.44,null,21,0.1,3.5,7.3,12.8]
[23.5,0.374,0.644,0.98,1.35,null,21.5,0.05,3.3,6.9,12.3]
[24.5,0.353,0.606,0.922,1.27,null,22,0.03,3.1,6.5,11.8]
[25.5,0.331,0.569,0.864,1.2,null,22.5,0.01,2.9,6.3,11.3]
[26.5,0.31,0.532,0.806,1.12,null,23,null,2.7,5.9,10.8]
[27.5,0.289,0.493,0.746,1.03,null,23.5,null,2.5,5.5,10.3]
[29,0.283,0.479,0.719,0.988,null,24,null,2.3,5.2,9.8]
[31,0.264,0.445,0.663,0.904,null,24.5,null,2.1,4.8,9.4]
[34,0.233,0.39,0.577,0.78,null,25,null,1.9,4.4,8.9]
[37,0.205,0.342,0.502,0.673,null,25.5,null,1.7,4.2,8.4]
[40,0.18,0.298,0.435,0.58,null,26,null,1.5,3.9,7.9]
[44.5,0.146,0.24,0.349,0.463,null,26.5,null,1.4,3.7,7.4]
[49,0.116,0.191,0.277,0.366,null,27,null,1.3,3.4,7]
[53.5,0.0907,0.149,0.215,0.284]
[58,0.0675,0.111,0.159,0.21]
[62.5,0.0445,0.0729,0.105,0.138]
[67,0.0194,0.0318,0.0457,0.0601]
[70,4.83e-31,4.84e-31,4.81e-31,4.79e-31]
[]
[]
[]
[]
[]
[]
["SelfSim",{"$nulls":5},"Proposed measurements"]
["Settlements(mm)",{"$nulls":5},"Settlements(mm)"]
["Distance from the wall (m)","Stage 2","Stage 3","Stage 4","Stage 5",null,"Distance from the wall (m)","Stage 2","Stage 3","Stage 4","Stage 5"]
[0,0.129,0.0192,-0.0952,-0.213,null,0]
[1.012,0.317,0.209,0.0878,-0.0259,null,1.012,0.5,1,1.7]
[2.077,0.407,0.324,0.216,0.108,null,2.077,1.2,1.8,2.9,3.5]
[3.1984,0.439,0.394,0.312,0.212,null,3.1984,1.4,2.1,3.9,4.5]
[4.3788,0.444,0.435,0.384,0.298,null,4.3788,1.8,2.4,4.6,5.8]
[5.6213,0.43,0.453,0.436,0.369,null,5.6213,1.9,2.6,5,6.3]
[6.9292,0.41,0.459,0.472,0.426,null,6.9292,2,2.7,5.3,6.6]
[8.306,0.385,0.454,0.494,0.471,null,8.306,1.95,2.65,5.35,6.6]
[9.7553,0.361,0.446,0.507,0.506,null,9.7553,1.85,2.5,5,6.25]
[11.281,0.338,0.433,0.512,0.532,null,11.281,1.7,2.3,4.5,5.7]
[12.887,0.318,0.421,0.515,0.553,null,12.887,1.45,2,3.9,5.1]
[14.577,0.3,0.409,0.513,0.568,null,14.577,1.3,1.8,3.4,4.5]
[16.356,0.285,0.399,0.512,0.582,null,16.356,1.15,1.5,2.85,4]
[18.229,0.272,0.389,0.509,0.592,null,18.229,1,1.3,2.4,3.4]
[20.201,0.262,0.382,0.508,0.601,null,20.201,0.7,1,1.95,2.9]
[22.276,0.254,0.375,0.506,0.608]
[24.46,0.247,0.37,0.504,0.615]
[26.76,0.241,0.366,0.503,0.619]
[29.18,0.236,0.362,0.501,0.622]
[31.728,0.232,0.358,0.498,0.623]
[34.41,0.227,0.353,0.494,0.622]
[37.234,0.223,0.349,0.489,0.618]
[40.205,0.218,0.343,0.483,0.612]
[43.333,0.214,0.337,0.475,0.604]
[46.626,0.209,0.33,0.466,0.594]
[50.092,0.203,0.321,0.455,0.581]
[53.741,0.197,0.312,0.442,0.565]
[57.581,0.191,0.302,0.429,0.548]
[61.624,0.184,0.292,0.414,0.53]
[65.879,0.177,0.281,0.398,0.51]
[70.359,0.169,0.269,0.382,0.49]
[75.074,0.162,0.258,0.366,0.468]
[80.037,0.155,0.246,0.349,0.448]
[85.262,0.148,0.235,0.333,0.427]
[90.761,0.141,0.225,0.318,0.408]
[96.55,0.135,0.215,0.305,0.39]
[102.64,0.13,0.206,0.292,0.374]
[109.06,0.126,0.199,0.282,0.361]
[115.81,0.122,0.194,0.274,0.351]
[122.92,0.12,0.19,0.269,0.344]
[130.4,0.119,0.189,0.267,0.342]

{"sheet":"Figure 17","index":7,"n_rows":116,"n_cols":11,"rows_kept":116,"cut":false,"hidden":false,"merged":[[0,0,1,10]],"flags":["formulas_cached_only"]}
["FIG.17. Computed deformations in Cluster 1 after six passes of SelfSim learning with Cluster 1 measured deformations; a) wall deformations, and b) surface settlements, Shanghai excavation"]
[]
[]
[null,"Wall deflection (mm)",{"$nulls":6},"Wall deflection (mm)"]
[null,null,"SelfSim",{"$nulls":5},"Proposed measurements"]
["Elevation (m)","Stage 2","Stage3","Stage4","Stage5",null,"Elevation (m)","Stage 2","Stage3","Stage4","Stage5"]
[0,0.397,0.343,0.403,0.413,null,0,0.4,0.4,0.4,0.4]
[0.5,0.932,0.845,0.873,0.895,null,0.5,0.5,0.5,0.5,0.5]
[1,1.47,1.35,1.34,1.38,null,1,0.7,0.7,0.7,0.7]
[1.5,2.01,1.86,1.82,1.87,null,1.5,0.9,0.9,0.9,0.9]
[2,2.55,2.37,2.3,2.36,null,2,1.1,1.1,1.1,1.1]
[2.5,3.05,2.87,2.77,2.83,null,2.5,1.4,1.4,1.4,1.4]
[3,3.52,3.37,3.24,3.3,null,3,1.6,1.6,1.6,1.6]
[3.5,3.95,3.87,3.71,3.76,null,3.5,1.9,1.9,1.9,1.9]
[4,4.32,4.37,4.2,4.24,null,4,2.3,2.3,2.3,2.3]
[4.5,4.64,4.91,4.73,4.74,null,4.5,2.7,2.7,2.7,2.7]
[5,4.9,5.48,5.32,5.28,null,5,3.2,3.2,3.2,3.2]
[5.5,5.1,6.06,5.95,5.87,null,5.5,3.5,3.9,3.9,3.9]
[6,5.23,6.61,6.62,6.48,null,6,3.8,4.7,4.7,4.7]
[6.5,5.31,7.11,7.33,7.12,null,6.5,3.9,5.6,5.6,5.6]
[7,5.34,7.55,8.08,7.8,null,7,3.8,6.6,6.6,6.6]
[7.5,5.32,7.91,8.84,8.5,null,7.5,3.7,7.2,7.4,7.4]
[8,5.26,8.19,9.56,9.18,null,8,3.5,7.8,8.4,8.4]
[8.5,5.16,8.38,10.2,9.85,null,8.5,3.3,8,9.4,9.4]
[9,5.03,8.49,10.7,10.5,null,9,3.2,8.2,10.2,10.2]
[9.5,4.87,8.52,11.2,11.1,null,9.5,3,8.3,11,11]
[10,4.7,8.47,11.5,11.8,null,10,2.9,8.2,11.8,11.9]
[10.5,4.52,8.36,11.7,12.4,null,10.5,2.7,8.1,12.2,12.8]
[11,4.32,8.18,11.8,13,null,11,2.6,7.8,12.7,14]
[11.5,4.12,7.96,11.8,13.5,null,11.5,2.4,7.6,13,15]
[12,3.92,7.68,11.7,13.8,null,12,2.2,7.3,13.1,16.4]
[12.5,3.72,7.38,11.5,14.1,null,12.5,2,7.1,13.2,17.2]
[13,3.51,7.05,11.2,14.2,null,13,1.8,6.8,13.1,17.7]
[13.5,3.31,6.7,10.8,14.2,null,13.5,1.6,6.6,12.9,18]
[14,3.12,6.33,10.4,14.1,null,14,1.4,6.4,12.7,18.1]
[14.5,2.93,5.97,10,13.9,null,14.5,1.3,6.1,12.3,18.2]
[15,2.75,5.6,9.54,13.6,null,15,1.2,5.9,11.9,18]
[15.5,2.58,5.25,9.07,13.3,null,15.5,1,5.7,11.5,17.7]
[16,2.42,4.92,8.6,12.9,null,16,0.9,5.5,11.1,17.4]
[16.5,2.28,4.62,8.17,12.5,null,16.5,0.8,5.3,10.7,17]
[17,2.16,4.36,7.77,12.1,null,17,0.7,5.1,10.3,16.6]
[17.5,2.06,4.14,7.44,11.8,null,17.5,0.6,4.9,9.9,16.2]
[18,1.98,3.97,7.15,11.5,null,18,0.5,4.7,9.5,15.7]
[18.5,1.91,3.83,6.92,11.2,null,18.5,0.4,4.5,9.1,15.2]
[19,1.86,3.71,6.71,10.9,null,19,0.35,4.3,8.8,14.8]
[19.5,1.81,3.61,6.53,10.6,null,19.5,0.3,4.1,8.4,14.3]
[20.5,1.72,3.43,6.19,10.1,null,20,0.25,3.9,8,13.8]
[21.5,1.63,3.24,5.82,9.53,null,20.5,0.2,3.7,7.6,13.3]
[22.5,1.52,3.01,5.39,8.86,null,21,0.1,3.5,7.3,12.8]
[23.5,1.41,2.76,4.89,8.08,null,21.5,0.05,3.3,6.9,12.3]
[24.5,1.29,2.5,4.38,7.26,null,22,0.03,3.1,6.5,11.8]
[25.5,1.18,2.25,3.89,6.43,null,22.5,0.01,2.9,6.3,11.3]
[26.5,1.07,2.01,3.41,5.61,null,23,null,2.7,5.9,10.8]
[27.5,0.966,1.77,2.94,4.77,null,23.5,null,2.5,5.5,10.3]
[29,0.895,1.62,2.62,4.06,null,24,null,2.3,5.2,9.8]
[31,0.767,1.37,2.14,3.2,null,24.5,null,2.1,4.8,9.4]
[34,0.511,0.898,1.36,1.92,null,25,null,1.9,4.4,8.9]
[37,0.249,0.415,0.611,0.835,null,25.5,null,1.7,4.2,8.4]
[40,0.217,0.359,0.521,0.7,null,26,null,1.5,3.9,7.9]
[44.5,0.171,0.282,0.403,0.529,null,26.5,null,1.4,3.7,7.4]
[49,0.133,0.218,0.307,0.398,null,27,null,1.3,3.4,7]
[53.5,0.102,0.165,0.231,0.296]
[58,0.0742,0.12,0.167,0.211]
[62.5,0.0485,0.0782,0.108,0.136]
[67,0.0212,0.0341,0.0468,0.0583]
[70,-4.83e-31,-4.81e-31,-4.79e-31,-4.77e-31]
[]
[]
[]
[]
[]
[]
["SelfSim",{"$nulls":5},"Proposed measurements"]
["Settlements(mm)",{"$nulls":5},"Settlements(mm)"]
["Distance from the wall (m)","Stage 2","Stage 3","Stage 4","Stage 5",null,"Distance from the wall (m)","Stage 2","Stage 3","Stage 4","Stage 5"]
[0,0.457,1.77,3.31,4.58,null,0]
[1.012,1.41,2.72,4.23,5.54,null,1.012,0.5,1,1.7]
[2.077,1.94,3.35,4.89,6.25,null,2.077,1.2,1.8,2.9,3.5]
[3.1984,2.22,3.73,5.33,6.74,null,3.1984,1.4,2.1,3.9,4.5]
[4.3788,2.33,3.87,5.51,6.98,null,4.3788,1.8,2.4,4.6,5.8]
[5.6213,2.3,3.85,5.51,7.01,null,5.6213,1.9,2.6,5,6.3]
[6.9292,2.21,3.71,5.34,6.85,null,6.9292,2,2.7,5.3,6.6]
[8.306,2.06,3.49,5.06,6.56,null,8.306,1.95,2.65,5.35,6.6]
[9.7553,1.91,3.24,4.73,6.18,null,9.7553,1.85,2.5,5,6.25]
[11.281,1.75,2.98,4.37,5.75,null,11.281,1.7,2.3,4.5,5.7]
[12.887,1.62,2.74,4.02,5.33,null,12.887,1.45,2,3.9,5.1]
[14.577,1.49,2.51,3.7,4.92,null,14.577,1.3,1.8,3.4,4.5]
[16.356,1.39,2.32,3.42,4.56,null,16.356,1.15,1.5,2.85,4]
[18.229,1.3,2.16,3.16,4.23,null,18.229,1,1.3,2.4,3.4]
[20.201,1.22,2.01,2.95,3.95,null,20.201,0.7,1,1.95,2.9]
[22.276,1.16,1.89,2.76,3.69]
[24.46,1.09,1.78,2.59,3.46]
[26.76,1.04,1.68,2.44,3.25]
[29.18,0.984,1.58,2.29,3.06]
[31.728,0.932,1.49,2.16,2.87]
[34.41,0.882,1.41,2.03,2.7]
[37.234,0.832,1.32,1.9,2.53]
[40.205,0.783,1.24,1.79,2.36]
[43.333,0.735,1.17,1.67,2.2]
[46.626,0.688,1.09,1.56,2.05]
[50.092,0.642,1.02,1.45,1.91]
[53.741,0.597,0.946,1.35,1.77]
[57.581,0.554,0.878,1.25,1.64]
[61.624,0.512,0.813,1.15,1.51]
[65.879,0.473,0.751,1.07,1.4]
[70.359,0.435,0.693,0.983,1.29]
[75.074,0.4,0.639,0.905,1.19]
[80.037,0.368,0.588,0.833,1.09]
[85.262,0.338,0.541,0.767,1]
[90.761,0.311,0.499,0.707,0.926]
[96.55,0.287,0.461,0.654,0.856]
[102.64,0.265,0.427,0.606,0.794]
[109.06,0.247,0.398,0.565,0.74]
[115.81,0.23,0.372,0.528,0.693]
[122.92,0.215,0.346,0.491,0.645]
[130.4,0.198,0.314,0.447,0.587]

{"sheet":"Figure 18","index":8,"n_rows":19,"n_cols":10,"rows_kept":19,"cut":false,"hidden":false,"merged":[[5,1,5,3],[0,0,0,9]],"flags":["formulas_cached_only"]}
["FIG.18. Comparison of predicted and measured pore water pressures for PA1 in cluster 1, Shanghai excavation"]
[]
["Predicted",{"$nulls":6},"Measured"]
["Pore pressure PA1 (kPa)",{"$nulls":6},"Pore pressure PA1 (kPa)"]
[{"$nulls":7},"Depths"]
[null,"Depths",{"$nulls":4},"Date","7.25m","10.5m","25.5m"]
["Date","7.25m","10.5m","25.5m",null,null,"2002-10-05",62.464728461639965,94.95593780211999,245.06539330969989]
["2002-11-06",37.743042,76.09655,238.57051,null,null,"2002-10-31",63.46584387155999,96.11732147822998,245.48958529929996]
["2002-11-08",30.525726,42.30014,248.10551,null,null,"2002-11-05",61.589636055359975,87.87242841888002,241.80043730250003]
["2002-11-24",43.409237,27.919714,242.16721,null,null,"2002-11-06",61.339842483840044,85.73084204343002,239.55409643519985]
["2002-12-21",50.258671,37.856678,220.85439,null,null,"2002-11-14",61.52717955651,75.8,227.90099234730005]
["2002-12-31",50.185837,45.28204,202.15446,null,null,"2002-12-19",42.91256520075001,47.150137428479965,190.2535093248]
[{"$nulls":6},"2002-12-30",35.83340273855998,15.182512301750002,142.53843866879993]
[{"$nulls":6},"2003-01-06",34.27030152356004,25.257745451430004,163.94883743999998]
[{"$nulls":6},"2003-01-11",32.531152150109975,30.89796504374999,175.7951657625]
[{"$nulls":6},"2003-01-15",33.01046356018995,30.759906701029934,177.04183645919997]
[{"$nulls":6},"2003-01-25",54.999320325960014,30.276896230919952,178.63005164999998]
[{"$nulls":6},"2003-01-31",56.48614976723994,30.276896230919952,179.53837929479994]
[{"$nulls":6},"2003-02-08",55.804299888749995,29.449579398120036,181.24301497529999]

{"sheet":"Figure 19","index":9,"n_rows":113,"n_cols":24,"rows_kept":113,"cut":false,"hidden":false,"merged":[[0,0,1,11]],"flags":["formulas_cached_only"]}
["FIG.19. Predicted deformations in cluster 2 after six passes of SelfSim learning with Cluster 1 deformations; a) wall deformations (I03 and I09) and b) surface settlement CJ02 and CJ05, (middle slab was used), Shanghai excavation"]
[]
[]
[null,"Wall deflection (mm)",{"$nulls":6},"Wall deflection (mm)",{"$nulls":6},"Wall deflection (mm)"]
[null,null,"Predicted",{"$nulls":5},"Measured I03",{"$nulls":6},"Measured I09"]
["Elevation (m)","Stage 2","Stage3","Stage4","Stage5",null,"Elevation (m)","Stage 2","Stage3","Stage4","Stage5",null,null,"Elevation (m)","Stage 2","Stage3","Stage4","Stage5"]
[0,0.415,0.334,0.407,0.407,null,0,-0.17,2.21,2.31,1.83,null,null,0,0.15,0.64,1.65,1.54]
[0.5,0.948,0.846,0.882,0.893,null,1,0.16,2.6,2.47,2.3,null,null,1,0.4,1.31,2.92,2.96]
[1,1.48,1.36,1.36,1.38,null,2,0.44,3.05,3,3.15,null,null,2,0.56,1.96,3.83,4.02]
[1.5,2.02,1.88,1.84,1.87,null,3,0.63,3.43,3.32,3.82,null,null,3,0.82,2.75,4.74,5.16]
[2,2.56,2.39,2.32,2.36,null,4,0.91,4.03,4.16,5.26,null,null,4,1.04,3.56,5.96,6.6]
[2.5,3.06,2.9,2.78,2.83,null,5,1.2,4.79,5.12,6.78,null,null,5,1.33,4.39,7.03,8.07]
[3,3.53,3.39,3.24,3.29,null,6,1.46,5.23,5.91,7.55,null,null,6,1.62,5.2,8.34,9.63]
[3.5,3.95,3.88,3.69,3.74,null,7,1.73,5.65,6.52,8.13,null,null,7,1.68,5.74,9.32,11.14]
[4,4.32,4.36,4.15,4.18,null,8,1.9,6.29,7.35,9.23,null,null,8,1.52,5.95,9.76,12.11]
[4.5,4.63,4.87,4.63,4.63,null,9,2.03,6.63,7.86,10.17,null,null,9,1.35,6.2,9.84,12.65]
[5,4.89,5.4,5.15,5.12,null,10,2.1,6.84,8.56,11.27,null,null,10,1.49,6.54,10.73,14.22]
[5.5,5.09,5.94,5.71,5.62,null,11,2.03,7.07,9.32,12.47,null,null,11,1.8,6.99,11.56,15.48]
[6,5.23,6.44,6.3,6.15,null,12,1.98,6.95,9.27,13.39,null,null,12,1.62,6.75,11.38,15.92]
[6.5,5.3,6.89,6.93,6.7,null,13,1.92,6.76,9.32,14.26,null,null,13,1.28,6.12,10.8,15.96]
[7,5.33,7.28,7.62,7.29,null,14,1.89,6.57,9.2,14.7,null,null,14,1.15,5.79,10.7,16.22]
[7.5,5.31,7.59,8.32,7.9,null,15,1.84,6.24,9.59,13.68,null,null,15,1.01,5.41,9.88,15.46]
[8,5.24,7.83,8.98,8.49,null,16,1.69,5.83,8.85,13.74,null,null,16,1.14,5.14,9.89,15.55]
[8.5,5.14,7.98,9.57,9.05,null,17,1.58,5.42,8.15,13.9,null,null,17,1.24,5.17,9.72,15.04]
[9,5.01,8.06,10.1,9.59,null,18,1.45,4.92,7.43,13.4,null,null,18,1.19,4.55,8.81,13.94]
[9.5,4.85,8.06,10.5,10.1,null,19,1.38,4.33,6.95,12.61,null,null,19,1,3.95,7.88,12.42]
[10,4.68,7.98,10.8,10.7,null,20,1.25,3.82,6.23,11.75,null,null,20,0.88,3.22,6.68,10.83]
[10.5,4.49,7.85,11,11.2,null,21,1.1,3.23,5.12,10.73,null,null,21,0.72,2.47,5.58,9.53]
[11,4.29,7.66,11,11.6,null,22,0.97,2.66,4.16,9.69,null,null,22,0.51,1.98,4.69,8.37]
[11.5,4.08,7.42,11,11.9,null,23,0.84,2.24,3.33,8.18,null,null,23,0.44,1.71,4.17,7.43]
[12,3.87,7.15,10.9,12.1,null,24,0.69,1.93,2.55,7.26,null,null,24,0.51,1.59,3.62,6.54]
[12.5,3.66,6.84,10.6,12.2,null,25,0.55,1.7,2.06,7.04,null,null,25,0.3,1.18,3.15,5.33]
[13,3.45,6.51,10.3,12.2,null,26,0.5,1.38,1.62,5.88,null,null,26,0.44,1.5,3.26,5.06]
[13.5,3.24,6.16,9.99,12.2,null,27,0.45,1.17,1.58,5.44,null,null,27,0.54,1.35,2.93,4.69]
[14,3.03,5.8,9.57,12,null,28,0.39,0.99,1.58,5.13,null,null,28,0.56,1.36,2.72,4.24]
[14.5,2.83,5.44,9.12,11.8,null,29,0.27,0.9,1.41,4.62,null,null,29,0.54,1.47,2.58,3.71]
[15,2.64,5.08,8.65,11.5,null,30,0.17,0.8,1.15,4.01,null,null,30,0.36,1.24,2.07,3.01]
[15.5,2.46,4.73,8.17,11.1,null,31,0.16,0.68,1.19,3.66,null,null,31,0.33,1.11,2.05,2.65]
[16,2.29,4.4,7.7,10.8,null,32,0.08,0.69,1.4,3.31,null,null,32,0.55,1.25,2.13,2.77]
[16.5,2.14,4.1,7.26,10.4,null,33,0.04,0.55,1.26,3.12,null,null,33,0.28,0.81,1.45,2.05]
[17,2.01,3.84,6.87,10.1,null,34,0.03,0.52,1.04,2.9,null,null,34,0.12,0.61,1.09,1.54]
[17.5,1.9,3.63,6.54,9.76]
[18,1.82,3.46,6.26,9.5]
[18.5,1.75,3.32,6.04,9.26]
[19,1.69,3.21,5.85,9.05]
[19.5,1.65,3.12,5.69,8.85]
[20.5,1.56,2.96,5.39,8.46]
[21.5,1.48,2.79,5.07,8]
[22.5,1.37,2.58,4.68,7.4]
[23.5,1.26,2.35,4.22,6.69]
[24.5,1.14,2.12,3.75,5.94]
[25.5,1.04,1.9,3.32,5.23]
[26.5,0.954,1.72,2.95,4.58]
[27.5,0.878,1.56,2.63,4]
[29,0.778,1.36,2.23,3.29]
[31,0.652,1.12,1.8,2.53]
[34,0.449,0.728,1.14,1.42]
[37,0.201,0.3,0.49,0.534]
[40,0.184,0.277,0.435,0.482]
[44.5,0.155,0.235,0.36,0.405]
[49,0.126,0.192,0.289,0.327]
[53.5,0.0992,0.151,0.225,0.256]
[58,0.0741,0.112,0.167,0.189]
[62.5,0.0493,0.0743,0.11,0.125]
[67,0.0218,0.0328,0.0485,0.0548]
[70,4.83e-31,4.81e-31,4.79e-31,4.76e-31]
[]
[]
[]
[null,"Settlement (mm)",{"$nulls":6},"Settlement (mm)",{"$nulls":9},"Settlement (mm)"]
[null,null,"Predicted",{"$nulls":5},"Measured CJ02",{"$nulls":9},"Measured CJ05"]
["Distance from the wall (m)","Stage 2","Stage3","Stage4","Stage5"]
[0,0.475,1.43,2.97,3.69,null,"Stage 2",null,"Stage3",null,"Stage4",null,"Stage5",null,null,null,"Stage 2",null,"Stage3",null,"Stage4",null,"Stage5"]
[1.012,1.41,2.36,3.85,4.6,null,"Distance from the wall (m)","Stage 2","Distance from the wall (m)","Stage 3","Distance from the wall (m)","Stage 4","Distance from the wall (m)","Stage 5",null,null,"Distance from the wall (m)","Stage 2","Distance from the wall (m)","Stage 3","Distance from the wall (m)","Stage 4","Distance from the wall (m)","Stage 5"]
[2.077,1.93,2.96,4.47,5.26,null,1.9278,0.14749,1.9962,2.0247,1.8868,3.0705,1.9278,6.8516,null,null,1.9679,0.75669,1.9353,3.8079,1.9679,4.1984,1.9027,4.5768]
[3.1984,2.2,3.31,4.85,5.7,null,4.9494,0.067042,4.9494,2.7889,4.9494,3.8482,4.9494,12.711,null,null,4.9915,1.074,4.9915,5.0161,4.9915,6.0413,4.9524,10.484]
[4.3788,2.29,3.42,4.98,5.91,null,9.0101,0.067042,8.976,2.0917,8.976,2.8694,9.0101,11.88,null,null,8.9924,0.63465,8.9924,3.3075,8.9599,4.0642,9.025,9.9835]
[5.6213,2.25,3.38,4.94,5.91,null,13.994,0,14.028,1.0458,14.028,1.3945,13.994,4.6125,null,null,14.016,0.37835,14.049,1.965,13.984,2.4165,14.016,7.0543]
[6.9292,2.14,3.21,4.73,5.73,null,19.975,0,20.051,0.63019,20.051,0.91176,20.051,2.6548]
[8.306,1.98,2.98,4.44,5.44]
[9.7553,1.81,2.72,4.1,5.06]
[11.281,1.64,2.46,3.74,4.66]
[12.887,1.49,2.22,3.39,4.25]
[14.577,1.36,2.01,3.08,3.87]
[16.356,1.25,1.82,2.8,3.53]
[18.229,1.15,1.67,2.56,3.23]
[20.201,1.07,1.54,2.36,2.98]
[22.276,1,1.43,2.19,2.76]
[24.46,0.941,1.34,2.04,2.57]
[26.76,0.887,1.26,1.91,2.4]
[29.18,0.839,1.18,1.8,2.25]
[31.728,0.794,1.12,1.69,2.11]
[34.41,0.751,1.05,1.59,1.98]
[37.234,0.709,0.994,1.49,1.85]
[40.205,0.668,0.935,1.4,1.73]
[43.333,0.628,0.878,1.31,1.62]
[46.626,0.588,0.822,1.22,1.51]
[50.092,0.549,0.768,1.14,1.4]
[53.741,0.511,0.715,1.06,1.29]
[57.581,0.474,0.663,0.981,1.19]
[61.624,0.438,0.614,0.908,1.1]
[65.879,0.404,0.566,0.837,1.01]
[70.359,0.372,0.522,0.771,0.93]
[75.074,0.341,0.479,0.709,0.852]
[80.037,0.313,0.44,0.652,0.781]
[85.262,0.287,0.404,0.599,0.716]
[90.761,0.263,0.371,0.551,0.657]
[96.55,0.243,0.342,0.508,0.604]
[102.64,0.224,0.316,0.47,0.557]
[109.06,0.208,0.293,0.438,0.518]
[115.81,0.194,0.273,0.409,0.482]
[122.92,0.181,0.253,0.379,0.446]
[130.4,0.165,0.227,0.342,0.399]

{"sheet":"Figure 20","index":10,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[[5,1,5,3],[0,0,0,9]],"flags":["formulas_cached_only"]}
["FIG.20. Comparison of predicted and measured pore water pressures for PA2 in cluster 2, Shanghai excavation"]
[]
["Predicted",{"$nulls":6},"Measured"]
["Pore pressure PA2 (kPa)",{"$nulls":6},"Pore pressure PA2 (kPa)"]
[{"$nulls":7},"Depths"]
[null,"Depths",{"$nulls":4},"Date","4m","7.5m","16m","24.5m"]
["Date","4m","7.5m","16m","24.5m",null,"2002-09-10",30.00933327872003,65.00744175908004,149.91753432832007,234.97285917183996]
["2002-11-03",8.8581038,46.409252,147.88947,240.77615,null,"2002-10-25",30.73760678875,65.96018011712,152.00967641872006,235.47641728]
["2002-11-14",31.902447,54.583427,138.46036,237.8501,null,"2002-11-01",31.002599735870078,66.096373329,148.97718006306997,234.3436308054399]
["2002-11-16",41.221333,60.48391,118.76932,242.92445,null,"2002-11-09",29.01731344307004,64.66743851463006,140.85629465875,225.18464146815998]
["2002-12-21",35.102325,73.349983,121.76812,226.7946,null,"2002-11-19",26.378021808670056,60.124620662120066,132.58092202675,209.869841368]
["2002-12-31",37.112896,75.585999,110.27197,205.44908,null,"2002-11-24",25.85122726546996,59.44869920192002,131.65334816127992,206.28051343743988]
[{"$nulls":6},"2002-12-05",25.193232735069913,59.516266673269946,132.58092202675,205.29179630975995]
[{"$nulls":6},"2002-12-10",22.960195655630045,57.01992208447993,133.09653845500003,206.28051343743988]
[{"$nulls":6},"2003-01-05",21.387790403629985,55.270224785,128.25813674706995,198.38823995776005]
[{"$nulls":6},"2003-01-12",21.060607665279967,55.942746624,123.33617775475,193.59845920095995]
[{"$nulls":6},"2003-01-20",19.75326184687998,50.17697810228008,108.78896636032005,170.83800205823985]
[{"$nulls":6},"2003-01-23",20.079890531229996,51.71501334087007,104.54939398299999,171.07962653055992]
[{"$nulls":6},"2003-01-28",20.21058078875,51.781950237319975,107.67715236042996,176.40522714496007]
[{"$nulls":6},"2003-02-04",21.911570893069914,55.20300275903008,110.91437745546997,178.58931980800003]
[{"$nulls":6},"2003-02-10",20.864364508750004,54.195330360680096,111.72504425082985,178.34648692095996]
[{"$nulls":6},"2003-02-17",20.798961204320044,54.39676614167003,112.637694895,179.07510252544012]

{"sheet":"Figure 21","index":11,"n_rows":113,"n_cols":14,"rows_kept":113,"cut":false,"hidden":false,"merged":[[0,0,1,11]],"flags":["formulas_cached_only"]}
["FIG.21. Predicted deformations in cluster 3 after six passes of SelfSim learning with cluster 1 deformations; a) wall deformations (I04) and b) surface settlement CJ06, (middle slab was used), Shanghai excavation"]
[]
[]
[null,"Wall deflection (mm)",{"$nulls":6},"Wall deflection (mm)"]
[null,null,"Predicted I04",{"$nulls":5},"Measured I04"]
["Elevation (m)","Stage 2","Stage3","Stage4","Stage5",null,"Elevation (m)","Stage 2","Stage3","Stage4","Stage5"]
[0,0.389,0.301,0.36,0.36,null,0,0.32,0,-0.3,0.13]
[0.5,0.925,0.815,0.841,0.85,null,1,0.64,0.83,0.81,1.3]
[1,1.46,1.33,1.32,1.34,null,2,0.97,1.78,1.99,2.51]
[1.5,2.01,1.85,1.81,1.84,null,3,1.31,2.88,3.32,3.93]
[2,2.54,2.37,2.3,2.33,null,4,1.62,3.95,4.56,5.12]
[2.5,3.05,2.88,2.77,2.81,null,5,1.91,5.07,5.72,6.11]
[3,3.52,3.38,3.25,3.28,null,6,2.17,6.1,7.01,7.64]
[3.5,3.94,3.87,3.72,3.75,null,7,2.23,6.72,7.98,8.54]
[4,4.32,4.37,4.2,4.22,null,8,2.3,7.43,9.03,10]
[4.5,4.64,4.89,4.72,4.72,null,9,2.4,7.85,9.77,11.05]
[5,4.89,5.44,5.29,5.25,null,10,2.43,8.12,10.45,12.11]
[5.5,5.09,6,5.9,5.83,null,11,2.43,8.19,10.98,13.13]
[6,5.23,6.53,6.55,6.42,null,12,2.36,8.09,10.94,13.62]
[6.5,5.31,7,7.23,7.04,null,13,2.27,7.81,10.79,13.59]
[7,5.34,7.42,7.97,7.7,null,14,2.13,7.34,10.35,13.27]
[7.5,5.32,7.76,8.7,8.37,null,15,1.97,6.76,9.94,13.21]
[8,5.25,8.02,9.39,9.03,null,16,1.77,6.06,9.01,12.23]
[8.5,5.15,8.19,10,9.65,null,17,1.52,5.22,8.23,11.71]
[9,5.02,8.29,10.5,10.2,null,18,1.27,4.32,7.25,10.79]
[9.5,4.87,8.31,11,10.8,null,19,1.01,3.36,6.01,9.45]
[10,4.7,8.25,11.3,11.4,null,20,0.76,2.43,4.79,7.94]
[10.5,4.51,8.13,11.5,11.9,null,21,0.55,1.56,4.09,7.25]
[11,4.32,7.96,11.5,12.4,null,22,0.36,0.88,3.49,6.33]
[11.5,4.11,7.73,11.5,12.7,null,23,0.16,0.48,3.05,5.51]
[12,3.91,7.46,11.4,12.9,null,24,0.07,0.23,2.81,4.75]
[12.5,3.7,7.16,11.2,13.1,null,25,0.03,0.09,2.51,4.04]
[13,3.5,6.83,10.9,13.1,null,26,0.01,0.06,2.46,3.64]
[13.5,3.29,6.49,10.6,13,null,27,-2.047e-16,0.02,2.09,3]
[14,3.1,6.13,10.2,12.9,null,28]
[14.5,2.9,5.77,9.72,12.6,null,29]
[15,2.72,5.41,9.27,12.4,null,30]
[15.5,2.55,5.07,8.8,12,null,31]
[16,2.39,4.74,8.35,11.7,null,32]
[16.5,2.24,4.45,7.92,11.3,null,33]
[17,2.12,4.19,7.54,11,null,34]
[17.5,2.02,3.97,7.21,10.7]
[18,1.94,3.8,6.93,10.4]
[18.5,1.87,3.66,6.7,10.2]
[19,1.82,3.55,6.5,9.92]
[19.5,1.77,3.45,6.32,9.7]
[20.5,1.68,3.27,5.99,9.25]
[21.5,1.59,3.09,5.64,8.74]
[22.5,1.49,2.87,5.21,8.1]
[23.5,1.37,2.62,4.73,7.36]
[24.5,1.25,2.37,4.23,6.57]
[25.5,1.14,2.13,3.74,5.76]
[26.5,1.04,1.89,3.27,4.96]
[27.5,0.933,1.66,2.8,4.14]
[29,0.868,1.53,2.52,3.55]
[31,0.741,1.29,2.05,2.81]
[34,0.484,0.814,1.27,1.64]
[37,0.221,0.338,0.533,0.618]
[40,0.195,0.3,0.461,0.536]
[44.5,0.156,0.239,0.36,0.418]
[49,0.122,0.187,0.277,0.32]
[53.5,0.093,0.142,0.209,0.241]
[58,0.0679,0.103,0.151,0.173]
[62.5,0.0443,0.0672,0.0973,0.111]
[67,0.0193,0.0291,0.0419,0.0476]
[70,-4.83e-31,-4.81e-31,-4.79e-31,-4.76e-31]
[]
[]
[]
[null,"Settlement (mm)",{"$nulls":6},"Settlement (mm)"]
[null,null,"Predicted CJ06",{"$nulls":5},"Measured CJ06"]
["Distance from the wall (m)","Stage 2","Stage3","Stage4","Stage5"]
[0,0.385,1.6,3.14,3.8,null,"Stage 2",null,"Stage3",null,"Stage4",null,"Stage5"]
[1.012,1.33,2.54,4.04,4.73,null,"Distance from the wall (m)","Stage 2","Distance from the wall (m)","Stage 3","Distance from the wall (m)","Stage 4","Distance from the wall (m)","Stage 5"]
[2.077,1.86,3.16,4.7,5.43,null,1.914,0.63766,1.9468,3.4458,1.9796,3.9608,2.0517,4.157]
[3.1984,2.14,3.51,5.11,5.9,null,4.9882,1.0178,4.9882,4.856,5.021,5.9351,4.9489,7.1491]
[4.3788,2.24,3.63,5.26,6.12,null,9.0129,0.77255,8.9801,4.0222,9.0129,4.7334,8.9801,6.8303]
[5.6213,2.21,3.59,5.23,6.14,null,14.034,0.38014,14.001,2.6855,14.067,3.2619,14.034,4.9786]
[6.9292,2.11,3.43,5.03,5.97,null,20.038,0.1962,20.005,1.6677,20.038,1.913,20.005,2.1705]
[8.306,1.96,3.2,4.75,5.68]
[9.7553,1.81,2.95,4.41,5.31]
[11.281,1.66,2.7,4.06,4.92]
[12.887,1.52,2.47,3.73,4.53]
[14.577,1.4,2.26,3.43,4.17]
[16.356,1.3,2.09,3.16,3.85]
[18.229,1.22,1.94,2.93,3.57]
[20.201,1.15,1.81,2.73,3.33]
[22.276,1.08,1.7,2.56,3.11]
[24.46,1.03,1.61,2.41,2.92]
[26.76,0.975,1.52,2.26,2.75]
[29.18,0.926,1.43,2.13,2.59]
[31.728,0.877,1.36,2.01,2.43]
[34.41,0.831,1.28,1.89,2.29]
[37.234,0.784,1.2,1.78,2.14]
[40.205,0.739,1.13,1.67,2.01]
[43.333,0.694,1.06,1.56,1.87]
[46.626,0.649,0.992,1.45,1.74]
[50.092,0.606,0.924,1.35,1.62]
[53.741,0.563,0.859,1.25,1.5]
[57.581,0.522,0.796,1.16,1.38]
[61.624,0.483,0.736,1.07,1.27]
[65.879,0.445,0.678,0.988,1.17]
[70.359,0.41,0.624,0.91,1.08]
[75.074,0.376,0.573,0.836,0.987]
[80.037,0.345,0.526,0.768,0.904]
[85.262,0.316,0.482,0.705,0.828]
[90.761,0.29,0.442,0.648,0.76]
[96.55,0.267,0.407,0.597,0.699]
[102.64,0.247,0.376,0.552,0.645]
[109.06,0.229,0.349,0.514,0.599]
[115.81,0.214,0.325,0.479,0.558]
[122.92,0.199,0.301,0.445,0.516]
[130.4,0.182,0.27,0.401,0.462]

{"sheet":"Figure 29","index":12,"n_rows":207,"n_cols":13,"rows_kept":207,"cut":false,"hidden":false,"merged":[[0,0,1,13]],"flags":["formulas_cached_only"]}
["FIG.29. Computed response after six passes of SelfSim learning with wall deformations (I-1) and inclinometer SI-4 at 22 m distance from the wall, down to fifth stage of the excavation using the database of SelfSim learning with wall deformations only down to stage 3; (a) surface settlements, (b) wall deflections (I-1), (c) lateral movement at SI-4 in TNEC excavation"]
[]
[]
[null,"Settlement (cm)",{"$nulls":7},"Settlement (cm)"]
[null,null,"SelfSim",{"$nulls":6},"Measured"]
["Distance from the wall (m)","Stage1","Stage 2","Stage3","Stage4","Stage5",null,"Distance from the wall (m)","Stage1","Stage 2","Stage3","Stage4","Stage5"]
[0,0.0246,0.0517,-0.114,-0.174,-0.176,null,0]
[0.73,-0.245,-0.569,-0.775,-1.08,-1.15,null,0.73]
[1.544,-0.374,-0.858,-1.35,-1.95,-2.08,null,1.544]
[2.4487,-0.466,-1.08,-1.8,-2.55,-2.72,null,2.4487]
[3.4487,-0.53,-1.23,-2.11,-3.01,-3.28,null,3.4487,null,null,-0.9,-1.5,-2.5]
[4.5687,-0.579,-1.33,-2.33,-3.39,-3.74,null,4.5687,null,null,-1.2,-1.95,-3]
[5.8087,-0.608,-1.39,-2.48,-3.66,-4.05,null,5.8087,null,null,-1.5,-2.4,-3.5]
[7.1887,-0.624,-1.42,-2.57,-3.84,-4.28,null,7.1887,null,null,-1.65,-2.7,-3.9]
[8.7187,-0.629,-1.43,-2.61,-3.93,-4.4,null,8.7187,null,null,-1.8,-3,-4.3]
[10.419,-0.624,-1.41,-2.6,-3.91,-4.37,null,10.419,null,null,-1.85,-3.2,-4.5]
[12.309,-0.611,-1.37,-2.55,-3.79,-4.23,null,12.309,null,null,-1.7,-3.15,-4.55]
[14.409,-0.59,-1.32,-2.46,-3.6,-3.99,null,14.409,null,null,-1.45,-2.9,-4.3]
[16.739,-0.563,-1.25,-2.32,-3.35,-3.7,null,16.739,null,null,-1.2,-2.5,-3.8]
[19.329,-0.53,-1.17,-2.16,-3.06,-3.35,null,19.329,null,null,-0.95,-2,-3]
[22.209,-0.492,-1.08,-1.96,-2.72,-2.95,null,22.209,null,null,-0.7,-1.5,-2.2]
[25.409,-0.45,-0.983,-1.75,-2.36,-2.53,null,25.409,null,null,-0.5,-1,-1.5]
[28.969,-0.405,-0.877,-1.52,-1.99,-2.12,null,28.969,null,null,-0.4,-0.6,-1]
[32.919,-0.357,-0.768,-1.3,-1.64,-1.73,null,32.919,null,null,null,-0.5,-0.8]
[37.319,-0.31,-0.661,-1.09,-1.34,-1.4,null,37.319,null,null,null,-0.4,-0.6]
[42.199,-0.264,-0.558,-0.894,-1.09,-1.13,null,42.199,null,null,null,-0.3,-0.5]
[47.619,-0.221,-0.462,-0.726,-0.878,-0.908,null,47.619,null,null,null,-0.2,-0.4]
[53.647,-0.18,-0.376,-0.583,-0.711,-0.739,null,53.647]
[60.347,-0.145,-0.3,-0.462,-0.575,-0.6,null,60.347]
[67.787,-0.114,-0.236,-0.363,-0.464,-0.49,null,67.787]
[76.057,-0.0879,-0.181,-0.28,-0.37,-0.392,null,76.057]
[85.247,-0.067,-0.138,-0.216,-0.292,-0.313,null,85.247]
[95.447,-0.0496,-0.102,-0.161,-0.225,-0.244,null,95.447]
[106.79,-0.0371,-0.0765,-0.122,-0.176,-0.192,null,106.79]
[119.39,-0.0274,-0.0565,-0.0903,-0.134,-0.149,null,119.39]
[133.39,-0.0217,-0.0449,-0.0741,-0.114,-0.129,null,133.39]
[148.95,-0.0168,-0.0341,-0.0549,-0.0867,-0.0987,null,148.95]
[]
[]
[]
[null,"Wall (cm)",{"$nulls":7},"Wall (cm)"]
[null,null,"SelfSim I-1",{"$nulls":6},"Measured I-1"]
["Elevation (m)","Stage1","Stage 2","Stage3","Stage4","Stage5",null,"Elevation (m)","Stage1","Stage 2","Stage3","Stage4","Stage5"]
[0,1.55,3.41,2.38,2,2.01,null,0]
[1,1.53,3.35,2.69,2.4,2.41,null,1,2.3,3.1,2.9,2.414,1.912]
[2,1.51,3.29,2.99,2.8,2.8,null,2,2.194,3.087,3.066,2.573,2.104]
[3,1.48,3.22,3.29,3.2,3.19,null,3,2.029,2.97,3.221,2.89,2.478]
[4,1.45,3.15,3.59,3.6,3.59,null,4,1.906,2.893,3.404,3.249,2.889]
[5,1.42,3.08,3.88,4.01,3.99,null,5,1.769,2.79,3.577,3.586,3.304]
[6,1.38,2.99,4.14,4.43,4.42,null,6,1.652,2.715,3.776,3.993,3.752]
[7,1.33,2.9,4.36,4.85,4.85,null,7,1.562,2.6,3.995,4.418,4.243]
[8,1.28,2.8,4.55,5.25,5.27,null,8,1.461,2.48,4.164,4.827,4.742]
[9,1.23,2.7,4.69,5.63,5.68,null,9,1.369,2.38,4.284,5.217,5.256]
[10,1.18,2.59,4.78,5.96,6.08,null,10,1.276,2.28,4.353,5.593,5.788]
[11,1.13,2.48,4.82,6.23,6.44,null,11,1.223,2.14,4.371,5.926,6.314]
[12,1.07,2.36,4.81,6.44,6.74,null,12,1.142,2.05,4.323,6.187,6.808]
[13,1.01,2.24,4.74,6.58,6.98,null,13,1.066,1.91,4.221,6.364,7.256]
[14,0.958,2.12,4.63,6.65,7.13,null,14,0.978,1.78,4.078,6.447,7.663]
[15,0.902,2,4.48,6.63,7.2,null,15,0.899,1.64,3.872,6.4,7.893]
[16,0.845,1.87,4.29,6.53,7.17,null,16,0.846,1.5,3.627,6.23,7.964]
[17,0.788,1.74,4.06,6.35,7.04,null,17,0.768,1.4,3.343,5.945,7.865]
[18,0.731,1.61,3.8,6.08,6.82,null,18,0.704,1.28,3.044,5.6,7.708]
[19,0.673,1.48,3.52,5.75,6.5,null,19,0.669,1.17,2.736,5.194,7.36]
[20,0.616,1.35,3.22,5.36,6.1,null,20,0.621,1.05,2.431,4.756,6.911]
[21,0.56,1.22,2.9,4.92,5.64,null,21,0.583,0.96,2.138,4.3,6.421]
[22,0.505,1.09,2.59,4.45,5.14,null,22,0.55,0.867,1.864,3.842,5.857]
[23,0.452,0.971,2.28,3.97,4.61,null,23,0.522,0.8,1.607,3.388,5.267]
[24,0.403,0.858,1.99,3.5,4.09,null,24,0.505,0.73,1.379,2.962,4.691]
[25,0.357,0.755,1.72,3.06,3.58,null,25,0.481,0.631,1.176,2.551,4.117]
[26,0.315,0.66,1.48,2.64,3.1,null,26,0.42,0.557,0.973,2.159,3.521]
[27,0.275,0.573,1.26,2.24,2.65,null,27,0.359,0.443,0.813,1.814,3.041]
[28,0.237,0.49,1.05,1.88,2.22,null,28,0.341,0.399,0.676,1.508,2.554]
[29,0.2,0.411,0.868,1.55,1.83,null,29,0.3,0.362,0.561,1.247,2.172]
[30,0.164,0.337,0.7,1.24,1.47,null,30,0.25,0.311,0.462,1.07,1.781]
[31,0.13,0.266,0.547,0.963,1.14,null,31,0.225,0.27,0.408,0.86,1.48]
[32,0.0985,0.201,0.41,0.717,0.844,null,32,0.2,0.22,0.358,0.714,1.182]
[33,0.0707,0.145,0.294,0.509,0.595,null,33,0.175,0.17,0.285,0.55,0.98]
[34,0.0485,0.0996,0.203,0.346,0.4,null,34,0.15,0.121,0.216,0.419,0.681]
[35,0.0435,0.0896,0.184,0.312,0.36,null,35,0.125,0.09,0.175,0.32,0.487]
[36,0.0414,0.0851,0.174,0.295,0.34,null,36,0.1,0.064,0.13,0.24,0.287]
[37,0.0392,0.0806,0.165,0.279,0.321,null,37,0.075,0.052,0.1,0.175,0.22]
[38,0.0376,0.0772,0.158,0.266,0.307,null,38,0.05,0.04,0.071,0.113,0.172]
[40,0.0344,0.0705,0.143,0.242,0.279,null,40,0.03,0.02,0.05,0.08,0.1]
[42,0.0314,0.0642,0.13,0.22,0.255,null,42,0.02,0.01,0.03,0.04,0.07]
[]
[]
[]
[null,"SI-4 (cm)",{"$nulls":7},"SI-4 (cm)"]
[null,null,"SelfSim I-1",{"$nulls":6},"Measured I-1"]
["Elevation (m)","Stage1","Stage 2","Stage3","Stage4","Stage5",null,"Elevation (m)","Stage1","Stage 2","Stage3","Stage4","Stage5"]
[0,0.797,1.74,2.49,2.64,2.68,null,0]
[1,0.783,1.71,2.44,2.57,2.6,null,1,0.208,0.769,1.094,2.009,2.7]
[2,0.767,1.67,2.39,2.57,2.6,null,2,0.182,0.735,1.059,1.752,2.44]
[3,0.751,1.62,2.35,2.6,2.64,null,3,0.15,0.692,0.965,1.566,2.24]
[4,0.732,1.58,2.29,2.63,2.69,null,4,0.136,0.666,0.899,1.449,1.99]
[5,0.713,1.52,2.23,2.65,2.74,null,5,0.117,0.631,0.839,1.35,1.85]
[6,0.691,1.46,2.14,2.63,2.74,null,6,0.109,0.6,0.816,1.25,1.78]
[7,0.669,1.4,2.03,2.57,2.7,null,7,0.103,0.549,0.759,1.15,1.69]
[8,0.645,1.33,1.9,2.44,2.59,null,8,0.097,0.499,0.73,1.05,1.68]
[9,0.631,1.31,1.91,2.43,2.58,null,9,0.093,0.463,0.697,0.92,1.51]
[10,0.616,1.29,1.93,2.47,2.61,null,10,0.088,0.436,0.64,0.84,1.42]
[11,0.599,1.27,1.96,2.51,2.65,null,11,0.075,0.377,0.546,0.727,1.34]
[12,0.581,1.24,1.98,2.53,2.67,null,12,0.063,0.357,0.506,0.681,1.18]
[13,0.561,1.2,2,2.56,2.7,null,13,0.052,0.334,0.467,0.62,1.14]
[14,0.54,1.16,2.02,2.63,2.77,null,14,0.044,0.32,0.41,0.56,1.02]
[15,0.517,1.12,2,2.62,2.76,null,15,0.027,0.29,0.35,0.512,0.91]
[16,0.492,1.07,1.94,2.49,2.6,null,16,0.01,0.26,0.319,0.426,0.74]
[17,0.463,1,1.86,2.44,2.55,null,17,0,0.23,0.284,0.343,0.63]
[18,0.432,0.933,1.75,2.31,2.43,null,18,0,0.2,0.253,0.31,0.51]
[19,0.401,0.861,1.62,2.16,2.27,null,19,0,0.17,0.216,0.27,0.47]
[20,0.369,0.787,1.49,2.01,2.12,null,20,0,0.14,0.16,0.25,0.42]
[21,0.336,0.71,1.36,1.85,1.96,null,21,0,0.12,0.12,0.23,0.37]
[22,0.302,0.63,1.2,1.67,1.78,null,22,0,0.1,0.1,0.19,0.32]
[23,0.268,0.548,1.03,1.46,1.57,null,23,0,0.08,0.08,0.17,0.29]
[24,0.232,0.464,0.847,1.22,1.31,null,24,0,0.06,0.06,0.131,0.25]
[25,0.217,0.431,0.792,1.15,1.25,null,25,0,0.04,0.04,0.1,0.22]
[26,0.2,0.398,0.733,1.07,1.17,null,26,0,0.02,0.02,0.08,0.18]
[27,0.183,0.364,0.672,0.993,1.09,null,27,0,0,0.01,0.06,0.12]
[28,0.166,0.329,0.61,0.911,1,null,28,0,0,0,0.03,0.08]
[29,0.147,0.293,0.546,0.826,0.912,null,29,0,0,0,0.01,0.04]
[30,0.128,0.255,0.48,0.736,0.817,null,30,0,0,0,0,0]
[31,0.109,0.217,0.411,0.638,0.713,null,31,0,0,0,0,0]
[32,0.0887,0.177,0.339,0.534,0.601,null,32,0,0,0,0,0]
[33,0.0678,0.136,0.263,0.422,0.479,null,33,0,0,0,0,0]
[34,0.0462,0.0933,0.185,0.303,0.348,null,34,0,0,0,0,0]
[35,0.0448,0.0905,0.18,0.296,0.34,null,35,0,0,0,0,0]
[36,0.0434,0.0877,0.175,0.288,0.332,null,36,0,0,0,0,0]
[37,0.042,0.0849,0.169,0.28,0.323,null,37,0,0,0,0,0]
[38,0.0406,0.0821,0.164,0.272,0.314,null,38,0,0,0,0,0]
[40,0.0379,0.0766,0.153,0.255,0.295,null,40,0,0,0,0,0]
[42,0.0353,0.0712,0.143,0.238,0.275,null,42,0,0,0,0,0]
{"$rows_empty":70}
[{"$nulls":8},35]
[{"$nulls":8},36]
[{"$nulls":8},37]
[{"$nulls":8},38]
[{"$nulls":8},40]
[{"$nulls":8},42]

{"sheet":"Figure 30","index":13,"n_rows":83,"n_cols":17,"rows_kept":83,"cut":false,"hidden":false,"merged":[[0,0,0,11]],"flags":["formulas_cached_only"]}
["FIG.30. Predicted and measured excavation response for a) lateral wall deflections, b) surface settlements in Formosa excavation"]
[]
[null,"Wall (cm)",{"$nulls":7},"Wall (cm)"]
[null,null,"Predicted",{"$nulls":6},"Measured"]
["Elevation (m)","Stage1","Stage 2","Stage3","Stage4","Stage5",null,"Elevation (m)","Deflection(cm)","Elevation (m)","Deflection(cm)","Elevation (m)","Deflection(cm)","Elevation (m)","Deflection(cm)","Elevation (m)","Deflection(cm)"]
[0,0.86831,1.8175,1.4178,0.70082,0.88012,null,-0.14044,1.883,-0.14864,2.1417,0.047359,1.1948,0.067861,0.5482,0.15356,0.4627]
[1,0.88404,1.8497,1.5787,1.1003,1.2213,null,0.60899,1.8032,0.67965,2.1919,0.70152,1.5022,0.96819,0.94395,0.56293,0.63867]
[2,0.89789,1.8794,1.7402,1.5005,1.5623,null,2.1079,1.6436,2.0901,2.2039,1.9365,1.8146,1.7924,1.1235,0.97092,0.85774]
[3,0.90702,1.9026,1.9026,1.9026,1.9026,null,3.2748,1.4811,4.2472,2.2224,3.5876,2.0874,2.5282,1.4747,1.3789,1.0768]
[4,0.9084,1.9151,2.067,2.3092,2.2427,null,4.3589,1.3179,5.659,2.1914,4.4104,2.31,3.098,1.8245,2.1161,1.3849]
[5,0.90106,1.914,2.2128,2.696,2.5715,null,5.6932,1.1137,6.826,2.0289,5.6508,2.45,3.7522,2.1319,2.7729,1.6062]
[6,0.88519,1.8978,2.3254,3.042,2.8809,null,6.7772,0.95056,8.2392,1.9547,6.6478,2.4154,4.3261,2.3524,3.1823,1.7821]
[7,0.86181,1.8662,2.3983,3.3306,3.1679,null,8.0272,0.78879,9.8224,1.7527,8.0582,2.4275,5.8044,2.8394,4.0868,2.0486]
[8,0.83232,1.8199,2.4296,3.5499,3.4353,null,9.6892,0.71678,11.238,1.5924,9.8032,2.3562,6.2138,3.0153,4.9041,2.4436]
[9,0.7982,1.7601,2.4213,3.6926,3.6926,null,10.939,0.55501,12.322,1.4292,11.055,2.1513,7.1182,3.2818,5.3923,2.7496]
[10,0.76083,1.6885,2.3771,3.7534,3.9551,null,12.185,0.52256,13.325,1.2222,12.22,2.0319,7.6935,3.4592,5.7201,2.8818]
[11,0.72137,1.6067,2.3013,3.7331,4.1832,null,13.266,0.44558,14.909,0.97704,13.389,1.8264,8.1831,3.7221,6.6273,3.062]
[12,0.68074,1.5165,2.1986,3.6365,4.3452,null,15.009,0.46049,15.993,0.81385,14.972,1.6243,9.0087,3.8585,7.6908,3.5454]
[13,0.63955,1.4197,2.0738,3.4732,4.4188,null,15.844,0.29517,17.16,0.65138,16.06,1.3318,9.6642,4.1228,8.3491,3.7235]
[14,0.59824,1.3181,1.9324,3.2561,4.3873,null,17.005,0.30512,19.406,0.49813,17.068,0.9524,11.156,4.1787,9.1705,3.9892]
[15,0.55702,1.2138,1.7798,2.9998,4.2557,null,19.663,0.24163,21.235,0.38444,18.485,0.74895,12.486,4.1038,9.7445,4.2097]
[16,0.51597,1.1087,1.6216,2.7201,4.0374,null,21.075,0.2106,22.401,0.26506,19.738,0.50097,13.405,3.9392,10.652,4.3899]
[17,0.47506,1.0053,1.464,2.4337,3.7551,null,22.235,0.26364,23.562,0.27501,21.317,0.42825,14.912,3.521,11.719,4.744]
[18,0.43415,0.90565,1.3127,2.1569,3.4348,null,23.478,0.3174,25.057,0.24468,22.234,0.30675,16.004,3.0991,12.379,4.879]
[19,0.39308,0.81134,1.172,1.9016,3.0988,null,25.06,0.15847,26.47,0.17054,23.562,0.27501,17.097,2.6342,13.376,4.8444]
[20,0.35166,0.7209,1.0393,1.6649,2.753,null,27.552,0.093566,27.633,0.13738,24.976,0.20087,18.36,2.0845,14.707,4.7265]
[21,0.3097,0.63234,0.91105,1.4413,2.4012,null,28.632,0.059693,28.632,0.059693,26.137,0.21081,19.702,1.6217,15.962,4.4354]
[22,0.26711,0.54414,0.78422,1.226,2.0468,null,30.126,0.02937,30.126,0.02937,27.466,0.17907,21.206,1.2896,17.059,3.8412]
[23,0.22394,0.45569,0.65738,1.0163,1.6933,null,31.042,-0.049029,31.621,-0.00095255,29.127,0.15016,22.22,0.7378,18.406,3.249]
[24,0.18063,0.36755,0.53106,0.81255,1.3475,null,32.122,-0.082902,null,0,30.041,0.11487,23.639,0.49124,19.835,2.6576]
[25,0.13828,0.28194,0.40844,0.61933,1.0211,null,33.78,-0.025594,null,0,31.454,0.040732,24.886,0.41568,21.019,1.9779]
[26,0.098983,0.20301,0.29545,0.44497,0.72951,{"$nulls":7},26.216,0.34083,22.108,1.6423]
[27,0.06636,0.13779,0.20206,0.30329,0.49493,{"$nulls":7},27.467,0.13596,23.531,1.2664]
[28,0.045514,0.096028,0.14216,0.21361,0.34742,{"$nulls":7},28.214,0.14235,24.789,0.84602]
[29,0.039007,0.082691,0.12274,0.18377,0.29887,{"$nulls":7},29.212,0.064664,26.041,0.64115]
[30,0.036716,0.077504,0.11495,0.17119,0.27821,{"$nulls":7},29.796,-0.016575,27.375,0.43699]
[31,0.035493,0.074477,0.11032,0.16344,0.26572,{"$nulls":7},30.377,-0.011605,28.464,0.10138]
[32,0.03454,0.072191,0.10684,0.15729,0.25626,{"$nulls":7},31.372,-0.0030829,29.795,0.02653]
[33,0.033219,0.069181,0.10227,0.1495,0.24448,{"$nulls":7},32.037,-0.040507,31.288,0.039312]
[34,0.032255,0.066738,0.098548,0.14351,0.23517,{"$nulls":9},31.62,0.042153]
[35,0.031283,0.064357,0.094946,0.13776,0.22642]
[36,0.030349,0.062097,0.091541,0.13239,0.21834]
[37,0.029431,0.059908,0.088257,0.12727,0.21069]
[38,0.028528,0.057788,0.085089,0.12236,0.20342]
[40,0.026766,0.053729,0.079049,0.11313,0.18977]
[42,0.02506,0.049884,0.073356,0.10454,0.17704]
[]
[]
[]
[null,"Settlement (cm)",{"$nulls":7},"Settlement (cm)"]
[null,null,"Predicted",{"$nulls":6},"Measured"]
["Distance from the wall (m)","Stage1","Stage 2","Stage3","Stage4","Stage5",null,"Distance from the wall (m)","Stage1","Stage 2","Stage3","Stage4","Stage5"]
[0,-0.011081,0.015809,0.075783,0.15228,0.15711,null,1.55,0,0.4,0.25,0.4,0.7]
[0.73,0.12771,0.34418,0.38124,0.39324,0.55331,null,3.55,0.22,0.92,0.82,1.42,2.2]
[1.544,0.20451,0.51617,0.58615,0.71359,1.0436,null,4.7,0.2,0.85,0.9,1.55,2.7]
[2.4487,0.2611,0.6461,0.77517,1.0444,1.5214,null,6.1,0.3,0.9,1.1,2,2.9]
[3.4487,0.30114,0.73637,0.92188,1.3323,1.9602,null,7.5,0.25,0.96,1.2,2.4,2.96]
[4.5687,0.33339,0.80653,1.0363,1.5701,2.3603,null,8.5,0.2,0.8,1.2,2.5,3.1]
[5.8087,0.35381,0.85157,1.1219,1.7528,2.6869,null,8.8,0.2,0.7,1.1,2.3,2.9]
[7.1887,0.36556,0.87739,1.1803,1.8791,2.9084,null,10.2,0.2,0.9,0.9,2.1,2.7]
[8.7187,0.37042,0.88623,1.2092,1.9437,2.9997,null,11.6,0,0.7,0.8,1.7,2.6]
[10.419,0.36861,0.87877,1.2105,1.9511,2.9477,null,12.9,0.1,0.9,0.7,1.6,2.4]
[12.309,0.36107,0.85654,1.1862,1.9053,2.7861,null,14.4,0.1,0.25,0.4,1.4,2.1]
[14.409,0.3483,0.82078,1.1375,1.8093,2.5433,null,16.4,0,0.4,0.35,0.9,1.4]
[16.739,0.33132,0.77384,1.0691,1.6758,2.2579,null,17.9,0,0.6,0.5,1.1,1.35]
[19.329,0.31034,0.71643,0.98208,1.5079,1.9395,null,19.4,0,0.45,0.5,0.9,1.4]
[22.209,0.28666,0.65228,0.88424,1.3239,1.6047,null,20.9,-0.15,0.6,0.4,1,1.1]
[25.409,0.26045,0.58208,0.77657,1.1264,1.2689,null,24,0,0.5,0.35,0.9,1.1]
[28.969,0.23331,0.51067,0.66873,0.9361,0.96553,null,25.5,-0.25,0.4,0.15,0.6,0.6]
[32.919,0.20533,0.43855,0.56134,0.75478,0.71434,null,27.1,0,0.45,0.2,0.4,0.4]
[37.319,0.17818,0.37043,0.46295,0.59811,0.52925,null,28.6,0.1,0.4,-0.2,0.2,0.3]
[42.199,0.1519,0.30663,0.37372,0.46567,0.40562,null,30.1,-0.1,0.4,0.1,0.2,0.3]
[47.619,0.12766,0.24969,0.2971,0.35975,0.32086,null,31.7,0,0.35,0.1,0.25,0.35]
[53.647,0.10559,0.2002,0.23352,0.27907,0.26638,null,33.3,-0.05,0.45,0.1,0.2,0.2]
[60.347,0.085947,0.15753,0.18051,0.21484,0.2219,null,34.8,-0.2,0.55,0.15,0.2,0.3]
[67.787,0.069175,0.12303,0.13971,0.16814,0.18707,null,36.2,-0.3,0.4,0.1,0.3,0.2]
[76.057,0.054631,0.093906,0.10589,0.12927,0.15356,null,37.6,-0.1,0.3,0.1,0.1,0.1]
[85.247,0.043095,0.072133,0.081632,0.10152,0.12573,null,38.9,-0.2,0.4,0,0.3,0.1]
[95.447,0.033401,0.054237,0.06187,0.078518,0.10217,null,40.4,-0.2,0.5,0.1,0.1,0.1]
[106.79,0.026489,0.042126,0.048793,0.062811,0.08444,null,41.9,0,0.6,0.1,0.3,0.3]
[119.39,0.021031,0.032784,0.03873,0.050523,0.069946,null,43.9,-0.1,0.4,0.15,0.2,0.1]
[133.39,0.01818,0.027782,0.033101,0.042917,0.060165,null,45.9,0,0.4,0.2,0.2,0.2]
[148.95,0.016643,0.023264,0.026886,0.032988,0.046833]