{"text_format":"2","workbook":"xls","n_sheets":10,"sheets":["Figure 3","Figure 4 ","Figure 5","Figure 6","Figure 7","Figure 8","Figure 9a","Figure 9b","Figure 13","Figure 14"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Figure 3","index":0,"n_rows":24,"n_cols":31,"rows_kept":24,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["Figure 3. General ground profile along with SPT N-values"]
[]
["Depth (m)",null,"BH1",null,"BH2",null,"BH3",null,"BH4",null,"BH5",null,"BH6",null,"BH7",null,"BH8",null,"BH9",null,"BH10",null,"BH11",null,"BH12",null,"BH13",null,"BH14",null,"Bh15"]
[null,"Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values","Elevation(m)","SPT N-values"]
[]
[]
[1,18.32,13,18.83,16,18.63,23,18.09,2,17.58,2,17.59,10,17.37,6,18.57,6,18.65,21,18.12,23,17.04,4,16.94,2,17.27,7,18.72,13,18.21,6]
[2,17.32,11,17.83,17,17.63,9,17.09,10,16.58,4,16.59,8,16.37,4,17.57,5,17.65,8,17.12,11,16.04,4,15.940000000000001,1,16.27,2,17.72,21,17.21,12]
[3,16.32,5,16.83,7,16.63,6,16.09,3,15.579999999999998,0,15.59,0,15.370000000000001,0,16.57,2,16.65,8,16.12,4,15.04,0,14.940000000000001,0,15.27,2,16.72,8,16.21,5]
[4,15.32,2,15.829999999999998,1,15.629999999999999,2,15.09,2,14.579999999999998,1,14.59,1,14.370000000000001,0,15.57,0,15.649999999999999,1,15.120000000000001,2,14.04,5,13.940000000000001,2,14.27,4,15.719999999999999,0,15.21,4]
[5,14.32,1,14.829999999999998,2,14.629999999999999,1,14.09,0,13.579999999999998,1,13.59,2,13.370000000000001,2,14.57,1,14.649999999999999,0,14.120000000000001,3,13.04,8,12.940000000000001,5,13.27,2,14.719999999999999,3,14.21,1]
[6.5,12.82,3,13.329999999999998,3,13.129999999999999,3,12.59,0,12.079999999999998,16,12.09,11,11.870000000000001,9,13.07,2,13.149999999999999,0,12.620000000000001,3,11.54,22,11.440000000000001,17,11.77,2,13.219999999999999,4,12.71,1]
[8,11.32,3,11.829999999999998,5,11.629999999999999,1,11.09,0,10.579999999999998,4,10.59,4,10.370000000000001,6,11.57,14,11.649999999999999,27,11.120000000000001,3,10.04,13,9.940000000000001,22,10.27,3,11.719999999999999,5,11.21,2]
[9.5,9.82,5,10.329999999999998,7,10.129999999999999,7,9.59,6,9.079999999999998,11,9.09,22,8.870000000000001,23,10.07,16,10.149999999999999,7,9.620000000000001,11,8.54,15,8.440000000000001,6,8.77,7,10.219999999999999,6,9.71,15]
[11,8.32,20,8.829999999999998,4,8.629999999999999,8,8.09,24,7.579999999999998,14,7.59,5,7.370000000000001,4,8.57,22,8.649999999999999,3,8.120000000000001,22,7.039999999999999,13,6.940000000000001,5,7.27,19,8.719999999999999,6,8.21,16]
[12.5,6.82,10,7.329999999999998,13,7.129999999999999,8,6.59,17,6.079999999999998,28,6.09,9,5.870000000000001,4,7.07,5,7.149999999999999,5,6.620000000000001,31,5.539999999999999,9,5.440000000000001,7,5.77,23,7.219999999999999,27,6.710000000000001,11]
[14,5.32,5,5.829999999999998,22,5.629999999999999,9,5.09,40,4.579999999999998,22,4.59,13,4.370000000000001,4,5.57,6,5.649999999999999,30,5.120000000000001,33,4.039999999999999,31,3.9400000000000013,29,4.27,27,5.719999999999999,20,5.210000000000001,25]
[15.5,3.8200000000000003,21,4.329999999999998,5,4.129999999999999,27,3.59,37,3.0799999999999983,35,3.09,31,2.870000000000001,33,4.07,4,4.149999999999999,44,3.620000000000001,36,2.539999999999999,17,2.4400000000000013,26,2.7699999999999996,28,4.219999999999999,38,3.710000000000001,30]
[17,2.3200000000000003,24,2.8299999999999983,33,2.629999999999999,29,2.09,29,1.5799999999999983,25,1.5899999999999999,40,1.370000000000001,34,2.5700000000000003,36,2.6499999999999986,33,2.120000000000001,38,1.0399999999999991,19,0.9400000000000013,29,1.2699999999999996,22,2.719999999999999,38,2.210000000000001,33]
[18.5,null,"--",1.3299999999999983,32,1.129999999999999,25,0.5899999999999999,34,0.0799999999999983,12,null,"--",null,null,1.0700000000000003,16,1.1499999999999986,29,0.620000000000001,8,null,"--",null,"--",-0.23000000000000043,7,null,"--",0.7100000000000009,23]
[19.94,null,null,-0.11000000000000298,34,-0.3100000000000023,8,null,null,-1.360000000000003,23,{"$nulls":4},-0.370000000000001,21,-0.2900000000000027,8,-0.8200000000000003,7,{"$nulls":4},-1.6700000000000017,7,null,null,-0.7300000000000004,10]
[21.5,{"$nulls":14},-1.9299999999999997,8,null,null,-2.379999999999999,8,{"$nulls":4},-3.2300000000000004,14]
[23,{"$nulls":14},-3.4299999999999997,10,null,null,-3.879999999999999,7,{"$nulls":4},-4.73,10]
[24.5,{"$nulls":14},-4.93,8,null,null,-5.379999999999999,7,{"$nulls":4},-6.23,14]

{"sheet":"Figure 4 ","index":1,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["Figure 4. Data points with respect to A-line"]
[]
["LL","PL","PI",null,"A-line"]
[45,26,19,null,"Plasticity","PI"]
[47,28,19,null,10,-7.3]
[32,23,9,null,100,58.4]
[56,31,25]
[43,27,16]
[43,28,15]
[48,29,19]
[47,27,20]
[51,30,21]
[41,25,16]
[44,27,17]
[42,27,15]

{"sheet":"Figure 5","index":2,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[[3,4,6,4],[3,1,6,1],[3,2,6,2],[0,0,0,4],[4,11,6,11],[4,17,6,17],[2,11,2,13],[3,9,6,9],[3,10,6,10],[3,0,6,0],[3,5,6,5],[3,6,6,6],[3,7,6,7]],"flags":["formulas_cached_only"]}
["Figure 5. Undrained shear strength versus water content"]
[]
["Laboratory Vane",null,null,null,"UU Triaxial Tests"]
["Natural water content (%)","Undrained Shear Strength (kN/m2)",null,null,"Water Content (%)","Undrained Shear Strength (kN/m2)"]
[]
[]
[]
[44.9,21]
[36.6,32]
[37.4,28]
[44.9,12]
[35.8,52]
[48.1,16,null,null,50.2,15]
[38.3,15]
[{"$nulls":4},45.8,7]
[39.3,30,null,null,40.4,30]
[37.6,19]
[51.1,9,null,null,43.35,15]
[34.9,56,null,null,34.6,100]
[38.7,36]
[31.8,17]
[]
[50,14]
[36.5,20]
[36.6,18]
[26.6,50]
[]
[39.4,22,null,null,38.35,24]

{"sheet":"Figure 6","index":3,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["Figure 6. Typical void ratio and coefficient of consolidation versus effective stress"]
[]
["Stress, kPa","e",null,"Avg. Stress, kPa","Cv (m2/yr)"]
[0,1.04068,null,6.25,7.27426]
[12.5,1.00946,null,18.75,5.78922]
[25,0.98762,null,37.5,4.95251]
[50,0.95619,null,75,5.91171]
[100,0.91742,null,150,7.16551]
[200,0.86722,null,300,7.57076]
[400,0.80518]
[200,0.816]
[100,0.82273]
[50,0.8362]
[10,0.87681]

{"sheet":"Figure 7","index":4,"n_rows":11,"n_cols":26,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["Figure 7. Coefficients of vertical consolidation against effective stresses"]
[]
[null,"BH1_UT1_V",null,null,"BH4_UT1_V",null,null,"BH5_UT3_V",null,null,"BH7_UT1_V",null,null,"BH9_UT1_V",null,null,"BH11_UT1_V",null,null,"BH12_UT1_V",null,null,"BH13_UT1_V",null,null,"BH14_UT1_V"]
[]
["Avg. Stress, kPa","Cv (m2/yr)",null,"Avg. Stress, kPa","Cv (m2/yr)",null,"Avg. Stress, kPa","Cv (m2/yr)",null,"Avg. Stress, kPa","Cv (m2/yr)",null,"Avg. Stress, kPa","Cv (m2/yr)",null,"Avg. Stress, kPa","Cv (m2/yr)",null,"Avg. Stress, kPa","Cv (m2/yr)",null,"Avg. Stress, kPa","Cv (m2/yr)"]
[6.25,58.99391,null,6.25,27.23974,null,6.25,7.7364,null,6.25,12.1373,null,6.25,4.28433,null,6.25,52.94129,null,6.25,5.30827,null,6.25,7.27426,null,6.25,20.8356]
[18.75,11.97049,null,18.75,18.46924,null,18.75,4.56997,null,18.75,7.39207,null,18.75,2.35412,null,18.75,66.98241,null,18.75,6.34587,null,18.75,5.78922,null,18.75,5.34623]
[37.5,16.78118,null,37.5,25.85754,null,37.5,5.38772,null,37.5,9.33864,null,37.5,1.97294,null,37.5,64.70863,null,37.5,3.88184,null,37.5,4.95251,null,37.5,6.48938]
[75,13.37942,null,75,36.63525,null,75,4.2143,null,75,7.47353,null,75,1.63857,null,75,76.29517,null,75,5.61531,null,75,5.91171,null,75,6.25393]
[150,15.45394,null,150,49.48366,null,150,5.0561,null,150,8.49709,null,150,2.5868,null,150,22.82688,null,150,6.18608,null,150,7.16551,null,150,7.68392]
[300,22.73582,null,300,56.21574,null,300,5.80479,null,300,8.20472,null,300,4.38085,null,300,38.11713,null,300,5.11398,null,300,7.57076,null,300,7.53449]

{"sheet":"Figure 8","index":5,"n_rows":11,"n_cols":8,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["Figure 8. Coefficients of horizontal consolidation versus effective stresses"]
[]
[null,"BH1_UT1_H",null,null,"BH12_UT1_H",null,null,"BH14_UT1_H"]
[]
["Avg. Stress, kPa","Ch (m2/yr)",null,"Avg. Stress, kPa","Ch (m2/yr)",null,"Avg. Stress, kPa","Ch (m2/yr)"]
[6.25,69.92503,null,6.25,17.08122,null,6.25,56.86149]
[18.75,16.80203,null,18.75,18.65436,null,18.75,63.77084]
[37.5,13.55337,null,37.5,12.62216,null,37.5,31.01031]
[75,13.13649,null,75,12.37518,null,75,31.25561]
[150,23.85681,null,150,16.08162,null,150,44.14763]
[300,31.04759,null,300,15.14468,null,300,30.45474]

{"sheet":"Figure 9a","index":6,"n_rows":10,"n_cols":26,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["Figure 9. Coefficients of permeability from laboratory tests a) Vertical"]
[]
[null,"BH1_UT1_V",null,null,"BH4_UT1_V",null,null,"BH5_UT3_V",null,null,"BH7_UT1_V",null,null,"BH9_UT1_V",null,null,"BH11_UT1_V",null,null,"BH12_UT1_V",null,null,"BH13_UT1_V",null,null,"BH14_UT1_V"]
["Avg. Stress, kPa","Kh (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kv (m/yr)"]
[6.25,0.7081503408,null,6.25,0.6454094687999999,null,6.25,0.19240838928,null,6.25,0.26377151904,null,6.25,0.15798179952,null,6.25,1.1671505136,null,6.25,0.18116265168,null,6.25,0.16436437056,null,6.25,2.2974795936]
[18.75,0.10205112672000001,null,18.75,0.20170961712000002,null,18.75,0.07553691936,null,18.75,0.1228737168,null,18.75,0.0492261192,null,18.75,0.7164411552,null,18.75,0.059859112320000005,null,18.75,0.059393956319999996,null,18.75,0.7015561632]
[37.5,0.10408330656,null,37.5,0.17024110416000002,null,37.5,0.06911934336,null,37.5,0.1123990344,null,37.5,0.027450132768000002,null,37.5,0.5242796928,null,37.5,0.04995333936,null,37.5,0.0551312352,null,37.5,0.408438504]
[75,0.0520139016,null,75,0.14482088064,null,75,0.037953576,null,75,0.062606844,null,75,0.013686024816,null,75,0.3721815648,null,75,0.04735729584,null,75,0.033990131519999994,null,75,0.19331536464000001]
[150,0.039679541279999994,null,150,0.13115853936,null,150,0.029644565328,null,150,0.044538923519999996,null,150,0.013001252112,null,150,0.06797805552,null,150,0.033291609119999996,null,150,0.031093865279999997,null,150,0.16669267344]
[300,0.03703997808,null,300,0.07441802208,null,300,0.018583660224,null,300,0.024161243327999998,null,300,0.012026663568,null,300,0.058533654239999997,null,300,0.016106885855999998,null,300,0.017401501728,null,300,0.0649436616]

{"sheet":"Figure 9b","index":7,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["Figure 9. Coefficients of permeability from laboratory tests b) Horizontal"]
[]
[null,"BH1_UT1_H",null,null,"BH12_UT1_H",null,null,"BH14_UT1_H"]
["Avg. Stress, kPa","Kv (m/yr)",null,"Avg. Stress, kPa","Kh (m/yr)",null,"Avg. Stress, kPa","Kh (m/yr)"]
[6.25,1.5086601648,null,6.25,0.67274172,null,6.25,1.011864096]
[18.75,0.15181556544,null,18.75,0.23883947279999998,null,18.75,0.09747241488000001]
[37.5,0.06692223024,null,37.5,0.13196018448000002,null,37.5,0.08306771616]
[75,0.06867657792,null,75,0.09395173584,null,75,0.045459459359999996]
[150,0.06609441024,null,150,0.08244645696,null,150,0.03535847856]
[300,0.05460206112,null,300,0.045892763999999996,null,300,0.01862027352]

{"sheet":"Figure 13","index":8,"n_rows":57,"n_cols":14,"rows_kept":57,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["Figure 13. Ground settlements with time"]
[]
[null,"Settlement plat numbers"]
["Elapsed time, days",10,9,8,7,6,5,4,3,2,1,11,12,22]
[0,180,135,260,150,100,140,42,76,180,275,108,141,297]
[1,180,140,260,150,100,158,47,96,188,280,132,152,300]
[2,185,155,272,150,143,169,60,108,198,283,141,159,302]
[3,190,170,290,152,155,183,60,134,200,288,152,165,306]
[4,190,175,290,157,157,191,null,149,212,288,155,169,308]
[5,205,175,290,162,165,202,92,149,215,288,164,180,310]
[6,220,195,307,162,168,207,106,149,216,293,171,182,310]
[7,222,195,308,null,null,213,106,162,219,293,184,182,315]
[8,231,202,317,184,192,213,113,175,228,293,184,188,321]
[9,231,203,317,194,204,213,120,176,231,295,184,189,326]
[10,231,203,317,197,204,226,120,187,234,297,187,199,326]
[11,231,203,320,197,209,227,120,193,241,305,190,203,352]
[12,null,null,null,207,220,232,123,193,242,310,194,203,355]
[13,242,219,334,207,220,237,129,198,242,310,199,210,358]
[14,246,225,343,207,220,237,132,205,243,310,199,210,369]
[15,251,225,344,212,226,244,137,213,243,310,202,213]
[16,251,225,345,219,239,246,143,215,243,316,207,215,374]
[17,257,234,354,242,242,248,143,224,246,317,207,215,376]
[18,257,234,354,251,251,249,146,229,248,317,208,215]
[19,258,234,354,261,261,254,148,236,254,317,214,215]
[20,258,234,354,232,261,256,151,240,260,317,216,217]
[21,258,236,357,232,262,260,151,245,260,317,220,221]
[22,258,236,358,233,264,261,151,246,260,318,221,221]
[23,258,244,362,237,272,261,152,246,260,319,221,221]
[24,263,245,368,237,272,261,154,252,263,320,221,221]
[25,263,246,369,241,280,261,157,254,263,320,221,221,385]
[26,263,247,370,242,281,262,159,254,263,321,221,null,388]
[27,263,248,371,242,285,262,159,259,263,null,221,226]
[28,264,252,374,244,289,262,159,259,null,325,221,228,390]
[29,264,252,374,245,293,263,162,263,null,325,222,229,396]
[30,264,252,377,245,293,274,162,265,null,326,231,null,398]
[31,264,252,375,245,293,276,162,265,null,null,234,null,399]
[32,264,252,376,245,295,276,163,268,null,null,234,229,400]
[33,264,253,377,245,295,276,183,null,null,329,234,229,400]
[34,264,254,376,246,297,276,183,null,null,329,234,null,400]
[35,264,254,378,250,301,279,186,null,null,null,239,null,402]
[36,264,254,378,250,302,280,186,null,null,null,239,null,405]
[37,267,257,385,250,303,280,188,null,null,null,239,null,405]
[38,267,257,385,250,305,280,{"$nulls":4},239]
[39,267,257,385,250,305,{"$nulls":7},407]
[40,270,261,386,254,309,{"$nulls":7},407]
[41,270,261,386,{"$nulls":9},407]
[42,270,261,387,{"$nulls":9},409]
[43,270,261,389,{"$nulls":9},410]
[44,270,261,389,{"$nulls":9},411]
[45,270,261,389,{"$nulls":9},415]
[46,{"$nulls":12},415]
[47,{"$nulls":12},415]
[48,{"$nulls":12},415]
[49,{"$nulls":12},415]
[50,{"$nulls":12},415]
[51,{"$nulls":12},415]
[52,{"$nulls":12},415]

{"sheet":"Figure 14","index":9,"n_rows":58,"n_cols":18,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Figure 14. Measured and predicted Degree of Consolidation"]
[]
[null,null,null,"Degree of consolidation"]
[null,"Settlement plat numbers"]
["Elapsed time, days",10,9,8,7,6,5,4,3,2,1,11,12,22,null,"Prediction"]
[0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[1,0.1,0.03968253968253968,0,0.12605042016806722,0,0.12857142857142856,0.03424657534246575,0.10416666666666667,0.0963855421686747,0.09259259259259259,0.183206106870229,0.125,0.08,null,null,"Smear","No. smear"]
[2,0.15,0.15873015873015872,0.09302325581395349,0.12605042016806722,0.20574162679425836,0.20714285714285716,0.1232876712328767,0.16666666666666666,0.21686746987951808,0.14814814814814814,0.25190839694656486,0.20454545454545456,0.096,null,"U","t","t"]
[3,0.2,0.2777777777777778,0.23255813953488372,0.14285714285714285,0.2631578947368421,0.30714285714285716,0.1232876712328767,0.3020833333333333,0.24096385542168675,0.24074074074074073,0.33587786259541985,0.2727272727272727,0.128,null,null,"days"]
[4,0.2,0.31746031746031744,0.23255813953488372,0.18487394957983194,0.2727272727272727,0.36428571428571427,null,0.3802083333333333,0.3855421686746988,0.24074074074074073,0.35877862595419846,0.3181818181818182,0.144,null,0.05,0.9789962772307063,0.4024368767352531]
[5,0.35,0.31746031746031744,0.23255813953488372,0.226890756302521,0.31100478468899523,0.44285714285714284,0.3424657534246575,0.3802083333333333,0.42168674698795183,0.24074074074074073,0.42748091603053434,0.4431818181818182,0.16,null,0.2,4.258972028080001,1.7507394470708655]
[6,0.5,0.47619047619047616,0.3643410852713178,0.226890756302521,0.3253588516746411,0.4785714285714286,0.4383561643835616,0.3802083333333333,0.43373493975903615,0.3333333333333333,0.48091603053435117,0.4659090909090909,0.16,null,0.4,9.749741948770946,4.007835157388885]
[7,0.52,0.47619047619047616,0.37209302325581395,null,null,0.5214285714285715,0.4383561643835616,0.4479166666666667,0.46987951807228917,0.3333333333333333,0.5801526717557252,0.4659090909090909,0.2,null,0.85,36.20889289407847,14.88442204045308]
[8,0.61,0.5317460317460317,0.4418604651162791,0.4117647058823529,0.44019138755980863,0.5214285714285715,0.4863013698630137,0.515625,0.5783132530120482,0.3333333333333333,0.5801526717557252,0.5340909090909091,0.248,null,0.9,43.94769844604129,18.065619771667162]
[9,0.61,0.5396825396825397,0.4418604651162791,0.4957983193277311,0.49760765550239233,0.5214285714285715,0.5342465753424658,0.5208333333333334,0.6144578313253012,0.37037037037037035,0.5801526717557252,0.5454545454545454,0.288,null,0.95,57.17727391869502,23.503913213199247]
[10,0.61,0.5396825396825397,0.4418604651162791,0.5210084033613446,0.49760765550239233,0.6142857142857143,0.5342465753424658,0.578125,0.6506024096385542,0.4074074074074074,0.6030534351145038,0.6590909090909091,0.288]
[11,0.61,0.5396825396825397,0.46511627906976744,0.5210084033613446,0.5215311004784688,0.6214285714285714,0.5342465753424658,0.609375,0.7349397590361446,0.5555555555555556,0.6259541984732825,0.7045454545454546,0.496]
[12,null,null,null,0.6050420168067226,0.5741626794258373,0.6571428571428571,0.5547945205479452,0.609375,0.7469879518072289,0.6481481481481481,0.6564885496183206,0.7045454545454546,0.52]
[13,0.72,0.6666666666666666,0.5736434108527132,0.6050420168067226,0.5741626794258373,0.6928571428571428,0.5958904109589042,0.6354166666666666,0.7469879518072289,0.6481481481481481,0.6946564885496184,0.7840909090909091,0.544]
[14,0.76,0.7142857142857143,0.6434108527131783,0.6050420168067226,0.5741626794258373,0.6928571428571428,0.6164383561643836,0.671875,0.7590361445783133,0.6481481481481481,0.6946564885496184,0.7840909090909091,0.632]
[15,0.81,0.7142857142857143,0.6511627906976745,0.6470588235294118,0.6028708133971292,0.7428571428571429,0.6506849315068494,0.7135416666666666,0.7590361445783133,0.6481481481481481,0.7175572519083969,0.8181818181818182]
[16,0.81,0.7142857142857143,0.6589147286821705,0.7058823529411765,0.6650717703349283,0.7571428571428571,0.6917808219178082,0.7239583333333334,0.7590361445783133,0.7592592592592593,0.7557251908396947,0.8409090909090909,0.672]
[17,0.87,0.7857142857142857,0.7286821705426356,0.8991596638655462,0.6794258373205742,0.7714285714285715,0.6917808219178082,0.7708333333333334,0.7951807228915663,0.7777777777777778,0.7557251908396947,0.8409090909090909,0.688]
[18,0.87,0.7857142857142857,0.7286821705426356,0.9747899159663865,0.722488038277512,0.7785714285714286,0.7123287671232876,0.796875,0.8192771084337349,0.7777777777777778,0.7633587786259542,0.8409090909090909]
[19,0.88,0.7857142857142857,0.7286821705426356,1.0588235294117647,0.7703349282296651,0.8142857142857143,0.726027397260274,0.8333333333333334,0.891566265060241,0.7777777777777778,0.8091603053435115,0.8409090909090909]
[20,0.88,0.7857142857142857,0.7286821705426356,0.8151260504201681,0.7703349282296651,0.8285714285714286,0.7465753424657534,0.8541666666666666,0.963855421686747,0.7777777777777778,0.8244274809160306,0.8636363636363636]
[21,0.88,0.8015873015873016,0.751937984496124,0.8151260504201681,0.7751196172248804,0.8571428571428571,0.7465753424657534,0.8802083333333334,0.963855421686747,0.7777777777777778,0.8549618320610687,0.9090909090909091]
[22,0.88,0.8015873015873016,0.7596899224806202,0.8235294117647058,0.784688995215311,0.8642857142857143,0.7465753424657534,0.8854166666666666,0.963855421686747,0.7962962962962963,0.8625954198473282,0.9090909090909091]
[23,0.88,0.8650793650793651,0.7906976744186046,0.8571428571428571,0.8229665071770335,0.8642857142857143,0.7534246575342466,0.8854166666666666,0.963855421686747,0.8148148148148148,0.8625954198473282,0.9090909090909091]
[24,0.93,0.873015873015873,0.8372093023255814,0.8571428571428571,0.8229665071770335,0.8642857142857143,0.7671232876712328,0.9166666666666666,1,0.8333333333333334,0.8625954198473282,0.9090909090909091]
[25,0.93,0.8809523809523809,0.8449612403100775,0.8907563025210085,0.861244019138756,0.8642857142857143,0.7876712328767124,0.9270833333333334,1,0.8333333333333334,0.8625954198473282,0.9090909090909091,0.76]
[26,0.93,0.8888888888888888,0.8527131782945736,0.8991596638655462,0.8660287081339713,0.8714285714285714,0.8013698630136986,0.9270833333333334,1,0.8518518518518519,0.8625954198473282,null,0.784]
[27,0.93,0.8968253968253969,0.8604651162790697,0.8991596638655462,0.8851674641148325,0.8714285714285714,0.8013698630136986,0.953125,1,null,0.8625954198473282,0.9659090909090909]
[28,0.94,0.9285714285714286,0.8837209302325582,0.9159663865546218,0.9043062200956937,0.8714285714285714,0.8013698630136986,0.953125,null,0.9259259259259259,0.8625954198473282,0.9886363636363636,0.8]
[29,0.94,0.9285714285714286,0.8837209302325582,0.9243697478991597,0.9234449760765551,0.8785714285714286,0.821917808219178,0.9739583333333334,null,0.9259259259259259,0.8702290076335878,1,0.848]
[30,0.94,0.9285714285714286,0.9069767441860465,0.9243697478991597,0.9234449760765551,0.9571428571428572,0.821917808219178,0.984375,null,0.9444444444444444,0.9389312977099237,null,0.864]
[31,0.94,0.9285714285714286,0.8914728682170543,0.9243697478991597,0.9234449760765551,0.9714285714285714,0.821917808219178,0.984375,null,null,0.9618320610687023,null,0.872]
[32,0.94,0.9285714285714286,0.8992248062015504,0.9243697478991597,0.9330143540669856,0.9714285714285714,0.8287671232876712,1,null,null,0.9618320610687023,1,0.88]
[33,0.94,0.9365079365079365,0.9069767441860465,0.9243697478991597,0.9330143540669856,0.9714285714285714,0.9657534246575342,null,null,1,0.9618320610687023,1,0.88]
[34,0.94,0.9444444444444444,0.8992248062015504,0.9327731092436975,0.9425837320574163,0.9714285714285714,0.9657534246575342,null,null,1,0.9618320610687023,null,0.88]
[35,0.94,0.9444444444444444,0.9147286821705426,0.9663865546218487,0.9617224880382775,0.9928571428571429,0.9863013698630136,null,null,null,1,null,0.896]
[36,0.94,0.9444444444444444,0.9147286821705426,0.9663865546218487,0.9665071770334929,1,0.9863013698630136,null,null,null,1,null,0.92]
[37,0.97,0.9682539682539683,0.9689922480620154,0.9663865546218487,0.9712918660287081,1,1,null,null,null,1,null,0.92]
[38,0.97,0.9682539682539683,0.9689922480620154,0.9663865546218487,0.9808612440191388,1,{"$nulls":4},1]
[39,0.97,0.9682539682539683,0.9689922480620154,0.9663865546218487,0.9808612440191388,{"$nulls":7},0.936]
[40,1,1,0.9767441860465116,1,1,{"$nulls":7},0.936]
[41,1,1,0.9767441860465116,{"$nulls":9},0.936]
[42,1,1,0.9844961240310077,{"$nulls":9},0.952]
[43,1,1,1,{"$nulls":9},0.96]
[44,1,1,1,{"$nulls":9},0.968]
[45,1,1,1,{"$nulls":9},1]
[46,{"$nulls":12},1]
[47,{"$nulls":12},1]
[48,{"$nulls":12},1]
[49,{"$nulls":12},1]
[50,{"$nulls":12},1]
[51,{"$nulls":12},1]
[52,{"$nulls":12},1]